,w##LENGTH##METERS,l##LENGTH##METERS,h##LENGTH##METERS,TK##OTHER##,TOC##OTHER##,SupEqui##OTHER##,Color##OTHER##,Weight##OTHER##,URL##OTHER##,Safety class##OTHER##,Degree of protection##OTHER##,Dimming/Balast##OTHER##,Lamp_0##OTHER##,Connection Load##ELECTRICAL_APPARENT_POWER##VOLT_AMPERES,CRI##OTHER##,Luminous flux of luminaire (lm)##OTHER##,Colour temperature (K)##OTHER##,Mat##OTHER##,SEO##OTHER##,SEO_outer##OTHER##,cutout_radius##LENGTH##METERS,Light Source##OTHER##
Inplana C07 CDP19 1000-830 ET 01,0.234,0,0.0417,10130565,6454940,Inplana_C07,Verkehrsweiß RAL 9016,1.07,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6454940,Schutzklasse II,,ET,LED,"9,5",80,999,3000,TRILUX_Alu_RAL_9016,TRILUX_CDP_Inplana_WH_3000,TRILUX_CDP_Inplana_WH_outer_3000,0.1075,Inplana_LS : TX044726
Inplana C07 CDP19 1000-830 ETDD 01,0.234,0,0.0417,10126200,6454951,Inplana_C07,Verkehrsweiß RAL 9016,1.07,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6454951,Schutzklasse II,,ETDD,LED,"9,5",80,999,3000,TRILUX_Alu_RAL_9016,TRILUX_CDP_Inplana_WH_3000,TRILUX_CDP_Inplana_WH_outer_3000,0.1075,Inplana_LS : TX044726
Inplana C07 CDP19 1000-830 ET 01 + C07 ZPF-T-T,0.234,0,0.0417,10130565,6454940,Inplana_C07 : Inplana_C07_ZPF-T,Verkehrsweiß RAL 9016,1.07,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6454940,Schutzklasse II,,ET,LED,"9,5",80,999,3000,TRILUX_Alu_RAL_9016,TRILUX_CDP_Inplana_WH_3000,TRILUX_CDP_Inplana_WH_outer_3000,0.123,Inplana_LS : TX045461
Inplana C07 CDP19 1000-830 ETDD 01 + C07 ZPF-T-T,0.234,0,0.0417,10126200,6454951,Inplana_C07 : Inplana_C07_ZPF-T,Verkehrsweiß RAL 9016,1.07,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6454951,Schutzklasse II,,ETDD,LED,"9,5",80,999,3000,TRILUX_Alu_RAL_9016,TRILUX_CDP_Inplana_WH_3000,TRILUX_CDP_Inplana_WH_outer_3000,0.123,Inplana_LS : TX045461
Inplana C07 CDP19 1000-830 ET 01 + C07 ZPF-T WR,0.234,0,0.0417,10130565,6454940,Inplana_C07 : Inplana_C07_ZPF-T_WR,Verkehrsweiß RAL 9016,1.07,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6454940,Schutzklasse II,,ET,LED,"9,5",80,999,3000,TRILUX_Alu_RAL_9016,TRILUX_CDP_Inplana_WH_3000,TRILUX_CDP_Inplana_WH_outer_3000,0.163,Inplana_LS : TX045462
Inplana C07 CDP19 1000-830 ETDD 01 + C07 ZPF-T WR,0.234,0,0.0417,10126200,6454951,Inplana_C07 : Inplana_C07_ZPF-T_WR,Verkehrsweiß RAL 9016,1.07,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6454951,Schutzklasse II,,ETDD,LED,"9,5",80,999,3000,TRILUX_Alu_RAL_9016,TRILUX_CDP_Inplana_WH_3000,TRILUX_CDP_Inplana_WH_outer_3000,0.163,Inplana_LS : TX045462
Inplana C07 CDP19 1000-840 ET 01,0.234,0,0.0417,10130564,6454840,Inplana_C07,Verkehrsweiß RAL 9016,1.07,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6454840,Schutzklasse II,,ET,LED,"9,5",80,1099,4000,TRILUX_Alu_RAL_9016,TRILUX_CDP_Inplana_WH_4000,TRILUX_CDP_Inplana_WH_outer_4000,0.1075,Inplana_LS : TX044727
Inplana C07 CDP19 1000-840 ETDD 01,0.234,0,0.0417,10126199,6454851,Inplana_C07,Verkehrsweiß RAL 9016,1.07,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6454851,Schutzklasse II,,ETDD,LED,"9,5",80,1099,4000,TRILUX_Alu_RAL_9016,TRILUX_CDP_Inplana_WH_4000,TRILUX_CDP_Inplana_WH_outer_4000,0.1075,Inplana_LS : TX044727
Inplana C07 CDP19 1000-840 ETDD 01 + C07 ZPF-T-T,0.234,0,0.0417,10126199,6454851,Inplana_C07 : Inplana_C07_ZPF-T,Verkehrsweiß RAL 9016,1.07,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6454851,Schutzklasse II,,ETDD,LED,"9,5",80,1099,4000,TRILUX_Alu_RAL_9016,TRILUX_CDP_Inplana_WH_4000,TRILUX_CDP_Inplana_WH_outer_4000,0.123,Inplana_LS : TX045463
Inplana C07 CDP19 1000-840 ET 01 + C07 ZPF-T-T,0.234,0,0.0417,10130564,6454840,Inplana_C07 : Inplana_C07_ZPF-T,Verkehrsweiß RAL 9016,1.07,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6454840,Schutzklasse II,,ET,LED,"9,5",80,1099,4000,TRILUX_Alu_RAL_9016,TRILUX_CDP_Inplana_WH_4000,TRILUX_CDP_Inplana_WH_outer_4000,0.123,Inplana_LS : TX045463
Inplana C07 CDP19 1000-840 ET 01 + C07 ZPF-T WR,0.234,0,0.0417,10130564,6454840,Inplana_C07 : Inplana_C07_ZPF-T_WR,Verkehrsweiß RAL 9016,1.07,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6454840,Schutzklasse II,,ET,LED,"9,5",80,1099,4000,TRILUX_Alu_RAL_9016,TRILUX_CDP_Inplana_WH_4000,TRILUX_CDP_Inplana_WH_outer_4000,0.163,Inplana_LS : TX045464
Inplana C07 CDP19 1000-840 ETDD 01 + C07 ZPF-T WR,0.234,0,0.0417,10126199,6454851,Inplana_C07 : Inplana_C07_ZPF-T_WR,Verkehrsweiß RAL 9016,1.07,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6454851,Schutzklasse II,,ETDD,LED,"9,5",80,1099,4000,TRILUX_Alu_RAL_9016,TRILUX_CDP_Inplana_WH_4000,TRILUX_CDP_Inplana_WH_outer_4000,0.163,Inplana_LS : TX045464
Inplana C07 OTA22 1000-830 ET 01,0.234,0,0.0417,10130563,6454740,Inplana_C07,Verkehrsweiß RAL 9016,0.94,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6454740,Schutzklasse II,,ET,LED,"9,5",80,1200,3000,TRILUX_Alu_RAL_9016,TRILUX_PMMA_Inplana_WH_3000,TRILUX_PMMA_Inplana_WH_3000,0.1075,Inplana_LS : TX044731
Inplana C07 OTA22 1000-830 ETDD 01,0.234,0,0.0417,10126198,6454751,Inplana_C07,Verkehrsweiß RAL 9016,0.94,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6454751,Schutzklasse II,,ETDD,LED,"9,5",80,1200,3000,TRILUX_Alu_RAL_9016,TRILUX_PMMA_Inplana_WH_3000,TRILUX_PMMA_Inplana_WH_3000,0.1075,Inplana_LS : TX044731
Inplana C07 OTA22 1000-830 ETDD 01 + C07 ZPF-T-T,0.234,0,0.0417,10126198,6454751,Inplana_C07 : Inplana_C07_ZPF-T,Verkehrsweiß RAL 9016,0.94,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6454751,Schutzklasse II,,ETDD,LED,"9,5",80,1200,3000,TRILUX_Alu_RAL_9016,TRILUX_PMMA_Inplana_WH_3000,TRILUX_PMMA_Inplana_WH_3000,0.123,Inplana_LS : TX045465
Inplana C07 OTA22 1000-830 ET 01 + C07 ZPF-T-T,0.234,0,0.0417,10130563,6454740,Inplana_C07 : Inplana_C07_ZPF-T,Verkehrsweiß RAL 9016,0.94,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6454740,Schutzklasse II,,ET,LED,"9,5",80,1200,3000,TRILUX_Alu_RAL_9016,TRILUX_PMMA_Inplana_WH_3000,TRILUX_PMMA_Inplana_WH_3000,0.123,Inplana_LS : TX045465
Inplana C07 OTA22 1000-830 ET 01 + C07 ZPF-T WR,0.234,0,0.0417,10130563,6454740,Inplana_C07 : Inplana_C07_ZPF-T_WR,Verkehrsweiß RAL 9016,0.94,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6454740,Schutzklasse II,,ET,LED,"9,5",80,1200,3000,TRILUX_Alu_RAL_9016,TRILUX_PMMA_Inplana_WH_3000,TRILUX_PMMA_Inplana_WH_3000,0.163,Inplana_LS : TX045466
Inplana C07 OTA22 1000-830 ETDD 01 + C07 ZPF-T WR,0.234,0,0.0417,10126198,6454751,Inplana_C07 : Inplana_C07_ZPF-T_WR,Verkehrsweiß RAL 9016,0.94,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6454751,Schutzklasse II,,ETDD,LED,"9,5",80,1200,3000,TRILUX_Alu_RAL_9016,TRILUX_PMMA_Inplana_WH_3000,TRILUX_PMMA_Inplana_WH_3000,0.163,Inplana_LS : TX045466
Inplana C07 OTA22 1000-840 ETDD 01,0.234,0,0.0417,10126197,6454651,Inplana_C07,Verkehrsweiß RAL 9016,0.94,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6454651,Schutzklasse II,,ETDD,LED,"9,5",80,1200,4000,TRILUX_Alu_RAL_9016,TRILUX_PMMA_Inplana_WH_4000,TRILUX_PMMA_Inplana_WH_4000,0.1075,Inplana_LS : TX044732
Inplana C07 OTA22 1000-840 ET 01,0.234,0,0.0417,10130562,6454640,Inplana_C07,Verkehrsweiß RAL 9016,0.94,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6454640,Schutzklasse II,,ET,LED,"9,5",80,1200,4000,TRILUX_Alu_RAL_9016,TRILUX_PMMA_Inplana_WH_4000,TRILUX_PMMA_Inplana_WH_4000,0.1075,Inplana_LS : TX044732
Inplana C07 OTA22 1000-840 ETDD 01 + C07 ZPF-T-T,0.234,0,0.0417,10126197,6454651,Inplana_C07 : Inplana_C07_ZPF-T,Verkehrsweiß RAL 9016,0.94,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6454651,Schutzklasse II,,ETDD,LED,"9,5",80,1200,4000,TRILUX_Alu_RAL_9016,TRILUX_PMMA_Inplana_WH_4000,TRILUX_PMMA_Inplana_WH_4000,0.123,Inplana_LS : TX045467
Inplana C07 OTA22 1000-840 ET 01 + C07 ZPF-T-T,0.234,0,0.0417,10130562,6454640,Inplana_C07 : Inplana_C07_ZPF-T,Verkehrsweiß RAL 9016,0.94,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6454640,Schutzklasse II,,ET,LED,"9,5",80,1200,4000,TRILUX_Alu_RAL_9016,TRILUX_PMMA_Inplana_WH_4000,TRILUX_PMMA_Inplana_WH_4000,0.123,Inplana_LS : TX045467
Inplana C07 OTA22 1000-840 ET 01 + C07 ZPF-T WR,0.234,0,0.0417,10130562,6454640,Inplana_C07 : Inplana_C07_ZPF-T_WR,Verkehrsweiß RAL 9016,0.94,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6454640,Schutzklasse II,,ET,LED,"9,5",80,1200,4000,TRILUX_Alu_RAL_9016,TRILUX_PMMA_Inplana_WH_4000,TRILUX_PMMA_Inplana_WH_4000,0.163,Inplana_LS : TX045468
Inplana C07 OTA22 1000-840 ETDD 01 + C07 ZPF-T WR,0.234,0,0.0417,10126197,6454651,Inplana_C07 : Inplana_C07_ZPF-T_WR,Verkehrsweiß RAL 9016,0.94,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6454651,Schutzklasse II,,ETDD,LED,"9,5",80,1200,4000,TRILUX_Alu_RAL_9016,TRILUX_PMMA_Inplana_WH_4000,TRILUX_PMMA_Inplana_WH_4000,0.163,Inplana_LS : TX045468
Inplana C07 OTA25 2000-830 ETDD 01,0.234,0,0.0417,10126202,6455151,Inplana_C07,Verkehrsweiß RAL 9016,0.94,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6455151,Schutzklasse II,,ETDD,LED,15,80,1900,3000,TRILUX_Alu_RAL_9016,TRILUX_PMMA_Inplana_WH_3000,TRILUX_PMMA_Inplana_WH_3000,0.1075,Inplana_LS : TX049210
Inplana C07 OTA25 2000-830 ET 01,0.234,0,0.0417,10130567,6455140,Inplana_C07,Verkehrsweiß RAL 9016,0.94,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6455140,Schutzklasse II,,ET,LED,15,80,1900,3000,TRILUX_Alu_RAL_9016,TRILUX_PMMA_Inplana_WH_3000,TRILUX_PMMA_Inplana_WH_3000,0.1075,Inplana_LS : TX049210
Inplana C07 OTA25 2000-830 ET 01 + C07 ZPF-T-T,0.234,0,0.0417,10130567,6455140,Inplana_C07 : Inplana_C07_ZPF-T,Verkehrsweiß RAL 9016,0.94,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6455140,Schutzklasse II,,ET,LED,15,80,1900,3000,TRILUX_Alu_RAL_9016,TRILUX_PMMA_Inplana_WH_3000,TRILUX_PMMA_Inplana_WH_3000,0.123,Inplana_LS : TX049214
Inplana C07 OTA25 2000-830 ETDD 01 + C07 ZPF-T-T,0.234,0,0.0417,10126202,6455151,Inplana_C07 : Inplana_C07_ZPF-T,Verkehrsweiß RAL 9016,0.94,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6455151,Schutzklasse II,,ETDD,LED,15,80,1900,3000,TRILUX_Alu_RAL_9016,TRILUX_PMMA_Inplana_WH_3000,TRILUX_PMMA_Inplana_WH_3000,0.123,Inplana_LS : TX049214
Inplana C07 OTA25 2000-830 ETDD 01 + C07 ZPF-T WR,0.234,0,0.0417,10126202,6455151,Inplana_C07 : Inplana_C07_ZPF-T_WR,Verkehrsweiß RAL 9016,0.94,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6455151,Schutzklasse II,,ETDD,LED,15,80,1900,3000,TRILUX_Alu_RAL_9016,TRILUX_PMMA_Inplana_WH_3000,TRILUX_PMMA_Inplana_WH_3000,0.163,Inplana_LS : TX049215
Inplana C07 OTA25 2000-830 ET 01 + C07 ZPF-T WR,0.234,0,0.0417,10130567,6455140,Inplana_C07 : Inplana_C07_ZPF-T_WR,Verkehrsweiß RAL 9016,0.94,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6455140,Schutzklasse II,,ET,LED,15,80,1900,3000,TRILUX_Alu_RAL_9016,TRILUX_PMMA_Inplana_WH_3000,TRILUX_PMMA_Inplana_WH_3000,0.163,Inplana_LS : TX049215
Inplana C07 OTA25 2000-830 ET EB3 01,0.234,0,0.0417,10139077,6688940,Inplana_C07,Verkehrsweiß RAL 9016,1.3,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6688940,,,ET,LED,20,80,1900,3000,TRILUX_Alu_RAL_9016,TRILUX_PMMA_Inplana_WH_3000,TRILUX_PMMA_Inplana_WH_3000,0.1075,Inplana_LS : TX048811
Inplana C07 OTA25 2000-840 ETDD 01,0.234,0,0.0417,10126201,6455051,Inplana_C07,Verkehrsweiß RAL 9016,0.94,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6455051,Schutzklasse II,,ETDD,LED,15,80,2000,4000,TRILUX_Alu_RAL_9016,TRILUX_PMMA_Inplana_WH_4000,TRILUX_PMMA_Inplana_WH_4000,0.1075,Inplana_LS : TX049211
Inplana C07 OTA25 2000-840 ET 01,0.234,0,0.0417,10130566,6455040,Inplana_C07,Verkehrsweiß RAL 9016,0.94,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6455040,Schutzklasse II,,ET,LED,15,80,2000,4000,TRILUX_Alu_RAL_9016,TRILUX_PMMA_Inplana_WH_4000,TRILUX_PMMA_Inplana_WH_4000,0.1075,Inplana_LS : TX049211
Inplana C07 OTA25 2000-840 ET 01 + C07 ZPF-T-T,0.234,0,0.0417,10130566,6455040,Inplana_C07 : Inplana_C07_ZPF-T,Verkehrsweiß RAL 9016,0.94,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6455040,Schutzklasse II,,ET,LED,15,80,2000,4000,TRILUX_Alu_RAL_9016,TRILUX_PMMA_Inplana_WH_4000,TRILUX_PMMA_Inplana_WH_4000,0.123,Inplana_LS : TX049216
Inplana C07 OTA25 2000-840 ETDD 01 + C07 ZPF-T-T,0.234,0,0.0417,10126201,6455051,Inplana_C07 : Inplana_C07_ZPF-T,Verkehrsweiß RAL 9016,0.94,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6455051,Schutzklasse II,,ETDD,LED,15,80,2000,4000,TRILUX_Alu_RAL_9016,TRILUX_PMMA_Inplana_WH_4000,TRILUX_PMMA_Inplana_WH_4000,0.123,Inplana_LS : TX049216
Inplana C07 OTA25 2000-840 ET 01 + C07 ZPF-T WR,0.234,0,0.0417,10130566,6455040,Inplana_C07 : Inplana_C07_ZPF-T_WR,Verkehrsweiß RAL 9016,0.94,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6455040,Schutzklasse II,,ET,LED,15,80,2000,4000,TRILUX_Alu_RAL_9016,TRILUX_PMMA_Inplana_WH_4000,TRILUX_PMMA_Inplana_WH_4000,0.163,Inplana_LS : TX049217
Inplana C07 OTA25 2000-840 ETDD 01 + C07 ZPF-T WR,0.234,0,0.0417,10126201,6455051,Inplana_C07 : Inplana_C07_ZPF-T_WR,Verkehrsweiß RAL 9016,0.94,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6455051,Schutzklasse II,,ETDD,LED,15,80,2000,4000,TRILUX_Alu_RAL_9016,TRILUX_PMMA_Inplana_WH_4000,TRILUX_PMMA_Inplana_WH_4000,0.163,Inplana_LS : TX049217
Inplana C07 OTA25 2000-840 ET EB3 01,0.234,0,0.0417,10139076,6688840,Inplana_C07,Verkehrsweiß RAL 9016,1.3,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6688840,,,ET,LED,20,80,2000,4000,TRILUX_Alu_RAL_9016,TRILUX_PMMA_Inplana_WH_4000,TRILUX_PMMA_Inplana_WH_4000,0.1075,Inplana_LS : TX048812
Inplana C09 CDP19 2000-830 ETDD 01,0.316,0,0.0417,10126206,6455551,Inplana_C09,Verkehrsweiß RAL 9016,1.69,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6455551,Schutzklasse II,,ETDD,LED,18,80,1698,3000,TRILUX_Alu_RAL_9016,TRILUX_CDP_Inplana_WH_3000,TRILUX_CDP_Inplana_WH_outer_3000,0.150,Inplana_LS : TX044738
Inplana C09 CDP19 2000-830 ET 01,0.316,0,0.0417,10130571,6455540,Inplana_C09,Verkehrsweiß RAL 9016,1.69,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6455540,Schutzklasse II,,ET,LED,18,80,1698,3000,TRILUX_Alu_RAL_9016,TRILUX_CDP_Inplana_WH_3000,TRILUX_CDP_Inplana_WH_outer_3000,0.150,Inplana_LS : TX044738
Inplana C09 CDP19 2000-830 ETDD 01 + C09 ZPF-T-T,0.316,0,0.0417,10126206,6455551,Inplana_C09 : Inplana_C09_ZPF-T,Verkehrsweiß RAL 9016,1.69,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6455551,Schutzklasse II,,ETDD,LED,18,80,1698,3000,TRILUX_Alu_RAL_9016,TRILUX_CDP_Inplana_WH_3000,TRILUX_CDP_Inplana_WH_outer_3000,0.163,Inplana_LS : TX045473
Inplana C09 CDP19 2000-830 ET 01 + C09 ZPF-T-T,0.316,0,0.0417,10130571,6455540,Inplana_C09 : Inplana_C09_ZPF-T,Verkehrsweiß RAL 9016,1.69,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6455540,Schutzklasse II,,ET,LED,18,80,1698,3000,TRILUX_Alu_RAL_9016,TRILUX_CDP_Inplana_WH_3000,TRILUX_CDP_Inplana_WH_outer_3000,0.163,Inplana_LS : TX045473
Inplana C09 CDP19 2000-840 ET 01,0.316,0,0.0417,10130570,6455440,Inplana_C09,Verkehrsweiß RAL 9016,1.69,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6455440,Schutzklasse II,,ET,LED,18,80,1798,4000,TRILUX_Alu_RAL_9016,TRILUX_CDP_Inplana_WH_4000,TRILUX_CDP_Inplana_WH_outer_4000,0.150,Inplana_LS : TX044739
Inplana C09 CDP19 2000-840 ETDD 01,0.316,0,0.0417,10126205,6455451,Inplana_C09,Verkehrsweiß RAL 9016,1.69,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6455451,Schutzklasse II,,ETDD,LED,18,80,1798,4000,TRILUX_Alu_RAL_9016,TRILUX_CDP_Inplana_WH_4000,TRILUX_CDP_Inplana_WH_outer_4000,0.150,Inplana_LS : TX044739
Inplana C09 CDP19 2000-840 ETDD 01 + C09 ZPF-T-T,0.316,0,0.0417,10126205,6455451,Inplana_C09 : Inplana_C09_ZPF-T,Verkehrsweiß RAL 9016,1.69,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6455451,Schutzklasse II,,ETDD,LED,18,80,1798,4000,TRILUX_Alu_RAL_9016,TRILUX_CDP_Inplana_WH_4000,TRILUX_CDP_Inplana_WH_outer_4000,0.163,Inplana_LS : TX045474
Inplana C09 CDP19 2000-840 ET 01 + C09 ZPF-T-T,0.316,0,0.0417,10130570,6455440,Inplana_C09 : Inplana_C09_ZPF-T,Verkehrsweiß RAL 9016,1.69,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6455440,Schutzklasse II,,ET,LED,18,80,1798,4000,TRILUX_Alu_RAL_9016,TRILUX_CDP_Inplana_WH_4000,TRILUX_CDP_Inplana_WH_outer_4000,0.163,Inplana_LS : TX045474
Inplana C09 OTA22 2000-830 ET 01,0.316,0,0.0417,10130569,6455340,Inplana_C09,Verkehrsweiß RAL 9016,1.43,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6455340,Schutzklasse II,,ET,LED,18,80,1900,3000,TRILUX_Alu_RAL_9016,TRILUX_PMMA_Inplana_WH_3000,TRILUX_PMMA_Inplana_WH_3000,0.150,Inplana_LS : TX044743
Inplana C09 OTA22 2000-830 ETDD 01,0.316,0,0.0417,10126204,6455351,Inplana_C09,Verkehrsweiß RAL 9016,1.43,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6455351,Schutzklasse II,,ETDD,LED,18,80,1900,3000,TRILUX_Alu_RAL_9016,TRILUX_PMMA_Inplana_WH_3000,TRILUX_PMMA_Inplana_WH_3000,0.150,Inplana_LS : TX044743
Inplana C09 OTA22 2000-830 ETDD 01 + C09 ZPF-T-T,0.316,0,0.0417,10126204,6455351,Inplana_C09 : Inplana_C09_ZPF-T,Verkehrsweiß RAL 9016,1.43,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6455351,Schutzklasse II,,ETDD,LED,18,80,1900,3000,TRILUX_Alu_RAL_9016,TRILUX_PMMA_Inplana_WH_3000,TRILUX_PMMA_Inplana_WH_3000,0.163,Inplana_LS : TX045475
Inplana C09 OTA22 2000-830 ET 01 + C09 ZPF-T-T,0.316,0,0.0417,10130569,6455340,Inplana_C09 : Inplana_C09_ZPF-T,Verkehrsweiß RAL 9016,1.43,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6455340,Schutzklasse II,,ET,LED,18,80,1900,3000,TRILUX_Alu_RAL_9016,TRILUX_PMMA_Inplana_WH_3000,TRILUX_PMMA_Inplana_WH_3000,0.163,Inplana_LS : TX045475
Inplana C09 OTA22 2000-840 ET 01,0.316,0,0.0417,10130568,6455240,Inplana_C09,Verkehrsweiß RAL 9016,1.43,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6455240,Schutzklasse II,,ET,LED,18,80,2000,4000,TRILUX_Alu_RAL_9016,TRILUX_PMMA_Inplana_WH_4000,TRILUX_PMMA_Inplana_WH_4000,0.150,Inplana_LS : TX044744
Inplana C09 OTA22 2000-840 ETDD 01,0.316,0,0.0417,10126203,6455251,Inplana_C09,Verkehrsweiß RAL 9016,1.43,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6455251,Schutzklasse II,,ETDD,LED,18,80,2000,4000,TRILUX_Alu_RAL_9016,TRILUX_PMMA_Inplana_WH_4000,TRILUX_PMMA_Inplana_WH_4000,0.150,Inplana_LS : TX044744
Inplana C09 OTA22 2000-840 ETDD 01 + C09 ZPF-T-T,0.316,0,0.0417,10126203,6455251,Inplana_C09 : Inplana_C09_ZPF-T,Verkehrsweiß RAL 9016,1.43,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6455251,Schutzklasse II,,ETDD,LED,18,80,2000,4000,TRILUX_Alu_RAL_9016,TRILUX_PMMA_Inplana_WH_4000,TRILUX_PMMA_Inplana_WH_4000,0.163,Inplana_LS : TX045476
Inplana C09 OTA22 2000-840 ET 01 + C09 ZPF-T-T,0.316,0,0.0417,10130568,6455240,Inplana_C09 : Inplana_C09_ZPF-T,Verkehrsweiß RAL 9016,1.43,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6455240,Schutzklasse II,,ET,LED,18,80,2000,4000,TRILUX_Alu_RAL_9016,TRILUX_PMMA_Inplana_WH_4000,TRILUX_PMMA_Inplana_WH_4000,0.163,Inplana_LS : TX045476
Inplana C09 OTA25 3000-830 ET 01,0.316,0,0.0417,10130573,6455740,Inplana_C09,Verkehrsweiß RAL 9016,1.43,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6455740,Schutzklasse II,,ET,LED,28,80,2999,3000,TRILUX_Alu_RAL_9016,TRILUX_PMMA_Inplana_WH_3000,TRILUX_PMMA_Inplana_WH_3000,0.150,Inplana_LS : TX049212
Inplana C09 OTA25 3000-830 ETDD 01,0.316,0,0.0417,10126208,6455751,Inplana_C09,Verkehrsweiß RAL 9016,1.43,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6455751,Schutzklasse II,,ETDD,LED,28,80,2999,3000,TRILUX_Alu_RAL_9016,TRILUX_PMMA_Inplana_WH_3000,TRILUX_PMMA_Inplana_WH_3000,0.150,Inplana_LS : TX049212
Inplana C09 OTA25 3000-830 ETDD 01 + C09 ZPF-T-T,0.316,0,0.0417,10126208,6455751,Inplana_C09 : Inplana_C09_ZPF-T,Verkehrsweiß RAL 9016,1.43,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6455751,Schutzklasse II,,ETDD,LED,28,80,2999,3000,TRILUX_Alu_RAL_9016,TRILUX_PMMA_Inplana_WH_3000,TRILUX_PMMA_Inplana_WH_3000,0.163,Inplana_LS : TX049218
Inplana C09 OTA25 3000-830 ET 01 + C09 ZPF-T-T,0.316,0,0.0417,10130573,6455740,Inplana_C09 : Inplana_C09_ZPF-T,Verkehrsweiß RAL 9016,1.43,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6455740,Schutzklasse II,,ET,LED,28,80,2999,3000,TRILUX_Alu_RAL_9016,TRILUX_PMMA_Inplana_WH_3000,TRILUX_PMMA_Inplana_WH_3000,0.163,Inplana_LS : TX049218
Inplana C09 OTA25 3000-840 ETDD 01,0.316,0,0.0417,10126207,6455651,Inplana_C09,Verkehrsweiß RAL 9016,1.43,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6455651,Schutzklasse II,,ETDD,LED,28,80,3099,4000,TRILUX_Alu_RAL_9016,TRILUX_PMMA_Inplana_WH_4000,TRILUX_PMMA_Inplana_WH_4000,0.150,Inplana_LS : TX049213
Inplana C09 OTA25 3000-840 ET 01,0.316,0,0.0417,10130572,6455640,Inplana_C09,Verkehrsweiß RAL 9016,1.43,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6455640,Schutzklasse II,,ET,LED,28,80,3099,4000,TRILUX_Alu_RAL_9016,TRILUX_PMMA_Inplana_WH_4000,TRILUX_PMMA_Inplana_WH_4000,0.150,Inplana_LS : TX049213
Inplana C09 OTA25 3000-840 ETDD 01 + C09 ZPF-T-T,0.316,0,0.0417,10126207,6455651,Inplana_C09 : Inplana_C09_ZPF-T,Verkehrsweiß RAL 9016,1.43,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6455651,Schutzklasse II,,ETDD,LED,28,80,3099,4000,TRILUX_Alu_RAL_9016,TRILUX_PMMA_Inplana_WH_4000,TRILUX_PMMA_Inplana_WH_4000,0.163,Inplana_LS : TX049219
Inplana C09 OTA25 3000-840 ET 01 + C09 ZPF-T-T,0.316,0,0.0417,10130572,6455640,Inplana_C09 : Inplana_C09_ZPF-T,Verkehrsweiß RAL 9016,1.43,http://www.trilux.de/trilux/openCatalog.do?Locale=de&ID=6455640,Schutzklasse II,,ET,LED,28,80,3099,4000,TRILUX_Alu_RAL_9016,TRILUX_PMMA_Inplana_WH_4000,TRILUX_PMMA_Inplana_WH_4000,0.163,Inplana_LS : TX049219
