IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "Project Number"
Time stamp: "2022-07-20T13:51:45"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20210416_1515(x64) - Exporter 19.2.30.41 - Alternate UI 19.2.30.41"
Application: "Autodesk Revit 2019 (ENG)" version "2019" identifier "Revit" by Organization "Autodesk Revit 2019 (ENG)"

People and organizations
  Person "Lana.Whittaker" of Organization (no name given)
  Owner history of Person "Lana.Whittaker" of Organization (no name given) | application "Autodesk Revit 2019 (ENG)" version "2019" identifier "Revit" by Organization "Autodesk Revit 2019 (ENG)" | change NOCHANGE | created 1658321505 (2022-07-20T12:51:45Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 51° 30′ 23.112487″ | longitude -0° 7′ 37.956022″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "London", "London", "United Kingdom"
      IFCBUILDINGSTOREY "Level 0" | long name "Level 0" | elevation 0.
        contains 1 element
          1 x IFCCOVERING | object type "NBS_HarlequinFloors_WoodFloatingFloorSystems_HarlequinFlexity:HarlequinFlexity" | FLOORING | names: "NBS_HarlequinFloors_WoodFloatingFloorSystems_HarlequinFlexity:HarlequinFlexity:316340" | material: "NBS_Concept" | property sets: BOS_General, NBS_Data, IFC, COBie

Property sets
  BOS_General | properties | on 1 object (1 IFCCOVERING)
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_HarlequinFloors_WoodFloatingFloorSystems_HarlequinFlexity" (IFCTEXT)
    ManufacturerName = "Harlequin Floors (British Harlequin plc)" (IFCTEXT)
    ManufacturerURL = "www.harlequinfloors.com" (IFCTEXT)
    NBSCertification = "www.nationalbimlibrary.com/cert/fbyoyy01" (IFCTEXT)
    ProductInformation = "n/a" (IFCTEXT)
    Uniclass2015Code = "Ss_30_20_95_95" (IFCTEXT)
    Uniclass2015Title = "Wood floating floor systems" (IFCTEXT)
    Uniclass2015Version = "Systems v1.22" (IFCTEXT)
    Version = "3" (IFCTEXT)
  BOS_General | properties | on 1 object (1 IFCBUILDING)
    Author = "" (IFCTEXT)
  NBS_Data | properties | on 1 object (1 IFCCOVERING)
    CategoryOfUse = "A4" (IFCTEXT)
    ContainsRedListMaterials = "n/a" (IFCTEXT)
    CountryOfMaterialOrigin = "n/a" (IFCTEXT)
    CountryOfProductManufacture = "n/a" (IFCTEXT)
    DynamicLoading = ">1500 N (69 kg/cm²)" (IFCTEXT)
    EmbodiedCarbon = "n/a" (IFCTEXT)
    Execution = "n/a" (IFCTEXT)
    FlooringBoardType = "Plywood" (IFCTEXT)
    FlooringJointing = "n/a" (IFCTEXT)
    InstallationMethod = "Tongue and groove" (IFCTEXT)
    Load = "1126 kN (229 kg/cm²)" (IFCTEXT)
    PerimeterFlankingSeal = "n/a" (IFCTEXT)
    ReactionToFire = "Class 3 BS 476-7 (Bfls1 with Standfast)" (IFCTEXT)
    Recyclability = "n/a" (IFCTEXT)
    RecycledContent = "n/a" (IFCTEXT)
    SamplesRequired = "n/a" (IFCTEXT)
    ShockAbsorption = "67%" (IFCTEXT)
    SubfloorPreparationLayer = "Smooth, flat, hard surface" (IFCTEXT)
    SystemAccessories = "n/a" (IFCTEXT)
    SystemCompletion = "n/a" (IFCTEXT)
    SystemPerformance = "n/a" (IFCTEXT)
    ThermalInsulation = "0.658 W/m²K" (IFCTEXT)
    ThermalResistance = "1.52 m²K/W" (IFCTEXT)
    TopLayer = "Engineered board with a hardwood layer" (IFCTEXT)
    Underlay = "Harlequin engineered board" (IFCTEXT)
    VapourControlLayer = "n/a" (IFCTEXT)
    WearLayer = "Harlequin performance vinyl" (IFCTEXT)
    Weight = "11.85 kg/m²" (IFCTEXT)
  IFC | properties | on 1 object (1 IFCCOVERING)
    IfcExportAs = "IfcCoveringType" (IFCTEXT)
    IfcExportType = "FLOORING" (IFCTEXT)
  COBie | properties | on 1 object (1 IFCCOVERING)
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Movable" (IFCTEXT)
    Category = "Ss_30_20_95_95:Wood floating floor systems" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "n/a" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "n/a" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Features = "n/a" (IFCTEXT)
    Finish = "n/a" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Manufacturer = "enquiries@harlequinfloors.com" (IFCTEXT)
    Material = "Plywood" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "HarlequinFlexity" (IFCTEXT)
    Name = "WoodFloatingFloorSystems_HarlequinFlexity_HarlequinFloors" (IFCTEXT)
    NominalHeight = 39. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 2250. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 1125. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "Rectangle" (IFCTEXT)
    Size = "n/a" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "Ten year" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  COBie | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCTEXT)
    Name = "Level 0" (IFCTEXT)
  COBie | properties | on 1 object (1 IFCBUILDING)
    Category = "Project Information" (IFCTEXT)