IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition[CoordinationView]"
Time stamp: "2022-07-13T10:34:51"
Author: "NBS"
Preprocessor: "Xbim.Ifc File Processor version 2.4.1.0"
Originating system: "Xbim version 2.4.1.0"
Authorization: "Add company name here"
Application: "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS"

People and organizations
  Person "NBS" of Organization "Add company name here"
  Owner history of Person "NBS" of Organization "Add company name here" | application "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS" | change ADDED | created 1657704891 (2022-07-13T09:34:51Z)
  Owner history of Person "NBS" of Organization "Add company name here" | application "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS" | change MODIFIED | created 1657704891 (2022-07-13T09:34:51Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  SOLIDANGLEUNIT: STERADIAN
  PLANEANGLEUNIT: RADIAN
  MASSUNIT: GRAM
  TIMEUNIT: SECOND
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  LUMINOUSINTENSITYUNIT: LUMEN

Spatial structure
IFCPROJECT "Add company name here"
  IFCSITE "Default site"
    IFCBUILDING "Default building"
      contains 1 element
        1 x IFCSLAB | type IFCSLABTYPE "NBS_HarlequinFloors_FoamBackedPolyvinylChloridePVCSheets_HarlequinAllegro" | FLOOR | names: "NBS_HarlequinFloors_FoamBackedPolyvinylChloridePVCSheets_HarlequinAllegro" | material: layers "NBS_HarlequinFloors_FoamBackedPolyvinylChloridePVCSheets_HarlequinAllegro" ("NBS_HarlequinFloors_FoamBackedPolyvinylChloridePVCSheets_HarlequinAllegro" 8.5) | property sets: COBie

Types
  IFCSLABTYPE "NBS_HarlequinFloors_FoamBackedPolyvinylChloridePVCSheets_HarlequinAllegro" | FLOOR | 1 occurrence | material: layers "NBS_HarlequinFloors_FoamBackedPolyvinylChloridePVCSheets_HarlequinAllegro" ("NBS_HarlequinFloors_FoamBackedPolyvinylChloridePVCSheets_HarlequinAllegro" 8.5) | property sets: xbim_MaterialFunctionAssignment, NBS_Data, COBie, BOS_General

Property sets
  COBie | properties | on 1 object (1 IFCSLAB)
    AssetIdentifier = "n/a" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Pr_35_57_71_32:Foam-backed polyvinyl chloride (PVC) sheets" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "Black,Grey" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "n/a" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Features = "n/a" (IFCTEXT)
    Finish = "Embossed" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Manufacturer = "enquiries@harlequinfloors.com" (IFCTEXT)
    Material = "Vinyl" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "HarlequinAllegro" (IFCTEXT)
    Name = "FoamBackedPolyvinylChloridePVCSheets_HarlequinAllegro_HarlequinFloors" (IFCTEXT)
    NominalHeight = 8.5 (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "n/a" (IFCTEXT)
    Size = "n/a" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "Ten year" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  xbim_MaterialFunctionAssignment | properties | on 1 type object
    MaterialFunctionAssignment (ifcpropertytablevalue)
  NBS_Data | properties | on 1 type object
    AbrasionResistance = "Group T, ≤ 2.00 mm³" (IFCTEXT)
    Accessories = "n/a" (IFCTEXT)
    Base = "Can be laid on any hard, smooth sub-floor" (IFCTEXT)
    ChemicalResistance = "Good Resistance. Not affected by dilute acids or domestic products" (IFCTEXT)
    ColourAndPattern = "Black.,Grey" (IFCTEXT)
    ContainsRedListMaterials = "n/a" (IFCTEXT)
    CountryOfMaterialOrigin = "n/a" (IFCTEXT)
    CountryOfProductManufacture = "n/a" (IFCTEXT)
    DimensionalStability = "≤ 0.40%" (IFCTEXT)
    EmbodiedCarbon = "n/a" (IFCTEXT)
    FixingType = "Adhesive.,Loose lay.,Tape" (IFCTEXT)
    FormaldehydeEmissions = "E1 Class < 0.10 mg/m³" (IFCTEXT)
    GlossLevel = "Nominal 6" (IFCTEXT)
    ImpactSoundReduction = "22 dB; with Activity: 24 dB" (IFCTEXT)
    LengthOptions = "10 m.,15 m.,18 m.,20 m.,25 m" (IFCTEXT)
    LightReflectance = "Black-2, Grey-21" (IFCTEXT)
    Lightfastness = "≥ 6" (IFCTEXT)
    ReactionToFire = "To 13501-1, Class Cfl-s1" (IFCTEXT)
    Recyclability = "100%" (IFCTEXT)
    RecycledContent = "23" (IFCTEXT)
    ResidualIndentation = "≤ 0.30 mm" (IFCTEXT)
    Seams = "Welded and taped" (IFCTEXT)
    SlipPotentialSlipResistanceValueSRVMinimumPendulumTestValuePTVMinimum = "n/a" (IFCTEXT)
    SlipPotentialSurfaceRoughnessRzMinimum = "n/a" (IFCTEXT)
    Standard = "TO BS EN ISO 10582" (IFCTEXT)
    ThirdPartyCertification = "Environmental Product Declaration A+" (IFCTEXT)
    UseClass = "n/a" (IFCTEXT)
    VOCEmissions = "≤ 100 µg/m³" (IFCTEXT)
    WearLayer = "0.65 mm" (IFCTEXT)
    Weight = "6 kg/m²" (IFCTEXT)
    Width = 1500. (IFCLENGTHMEASURE) [MILLI METRE]
  BOS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_HarlequinFloors_FoamBackedPolyvinylChloridePVCSheets_HarlequinAllegro" (IFCTEXT)
    ManufacturerName = "Harlequin Floors (British Harlequin plc)" (IFCTEXT)
    ManufacturerURL = "www.harlequinfloors.com" (IFCTEXT)
    NBSCertification = "www.nationalbimlibrary.com/cert/kxbzx43j" (IFCTEXT)
    ProductInformation = "n/a" (IFCTEXT)
    Uniclass2015Code = "Pr_35_57_71_32" (IFCTEXT)
    Uniclass2015Title = "Foam-backed polyvinyl chloride (PVC) sheets" (IFCTEXT)
    Uniclass2015Version = "Products v1.22" (IFCTEXT)
    Version = "2" (IFCTEXT)