IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "0001"
Time stamp: "2018-08-01T19:06:38"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20171027_0315(x64) - Exporter 17.0.1150.0 - Alternate UI 17.19.0.0"
Application: "Autodesk Revit 2017 (ENU)" version "2017" identifier "Revit" by Organization "Autodesk Revit 2017 (ENU)"

People and organizations
  Person "m" of Organization (no name given)
  Owner history of Person "m" of Organization (no name given) | application "Autodesk Revit 2017 (ENU)" version "2017" identifier "Revit" by Organization "Autodesk Revit 2017 (ENU)" | change NOCHANGE | created 1533139761 (2018-08-01T16:09:21Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "0001" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 21′ 30.344238″ | longitude -71° 3′ 35.194702″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "<Default>"
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | elevation 0.
        contains 1 element
          1 x IFCROOF | object type "gorter_RHTEI_verzamelbestand:RHTEI7090:308425" | names: "gorter_RHTEI_verzamelbestand:RHTEI7090:306675" | material: materials ("Gorter_Material 2", "Gorter_Material 1") | property sets: Pset_RoofCommon, Pset_ManufacturerTypeInformation, Constraints, Dimensions, Identity Data, Other

Property sets
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
    Client Name = "Owner" (IFCTEXT)
    Project Address = "Enter address here" (IFCTEXT)
    Project Issue Date = "Issue Date" (IFCTEXT)
    Project Name = "Project Name" (IFCTEXT)
    Project Number = "0001" (IFCTEXT)
    Project Status = "Project Status" (IFCTEXT)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Other | properties | on 1 object (1 IFCROOF)
    Category = "Windows" (IFCLABEL)
    Family = "gorter_RHTEI_verzamelbestand: RHTEI7090" (IFCLABEL)
    Family and Type = "gorter_RHTEI_verzamelbestand: RHTEI7090" (IFCLABEL)
    Host Id = "Basic Roof: Generic - 400mm" (IFCLABEL)
    Type = "gorter_RHTEI_verzamelbestand: RHTEI7090" (IFCLABEL)
    Type Id = "gorter_RHTEI_verzamelbestand: RHTEI7090" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: 8mm Head" (IFCLABEL)
    Family and Type = "Level: 8mm Head" (IFCLABEL)
    Type = "Level: 8mm Head" (IFCLABEL)
    Type Id = "Level: 8mm Head" (IFCLABEL)
  Other | properties | on 1 object (1 IFCROOF)
    Category = "Windows" (IFCLABEL)
    Family Name = "gorter_RHTEI_verzamelbestand" (IFCTEXT)
    Weight (kg) = 134. (IFCREAL)
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "gorter_RHTEI_verzamelbestand:RHTEI7090" (IFCIDENTIFIER)
    TotalArea = 2.92119037795703 (IFCAREAMEASURE) [SQUARE_METRE]
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCROOF)
    Manufacturer = "Gorter" (IFCLABEL)
  Constraints | properties | on 1 object (1 IFCROOF)
    Level = "Level: Level 1" (IFCLABEL)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Dimensions | properties | on 1 object (1 IFCROOF)
    Area = 2.92119037795703 (IFCAREAMEASURE) [SQUARE_METRE]
    Offset to structural layer = 50. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 0.155821111037555 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCROOF)
    A = 700. (IFCLENGTHMEASURE) [MILLI METRE]
    B = 900. (IFCLENGTHMEASURE) [MILLI METRE]
    Height = 900. (IFCLENGTHMEASURE) [MILLI METRE]
    Rough Height = 900. (IFCLENGTHMEASURE) [MILLI METRE]
    Rough Width = 700. (IFCLENGTHMEASURE) [MILLI METRE]
    Width = 700. (IFCLENGTHMEASURE) [MILLI METRE]
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Author = "" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCROOF)
    Mark = "1" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = FALSE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 object (1 IFCROOF)
    Assembly Code = "37.22.28" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Belastbaarheid = "" (IFCTEXT)
    Bestendigheid tegen sneeuwbelasting = "405 kg/m²" (IFCTEXT)
    Bestendigheid tegen windbelasting = "3000 Pa" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Constructiesterkte = "± 3000 Pa" (IFCTEXT)
    Geluidwerendheid = "27 dB" (IFCTEXT)
    Hard body impact test (EN 356) = "Class P5A" (IFCTEXT)
    Isolatiewaarde deksel = "Rc = 4,52 (m2.K)W; U = 0,221 W/(m2.K)" (IFCTEXT)
    Isolatiewaarde opstand = "Rc = 4,41 (m2.K)W; U = 0,227 W/(m2.K)" (IFCTEXT)
    Luchtdichtheid = "0,5 m3/hm1" (IFCTEXT)
    Manufacturer = "Gorter" (IFCTEXT)
    Model = "RHTEI" (IFCTEXT)
    OmniClass Number = "" (IFCTEXT)
    OmniClass Title = "" (IFCTEXT)
    Soft body impact test (EN 13049) = "Class 5" (IFCTEXT)
    Type Mark = "26" (IFCTEXT)
    Type Name = "RHTEI7090" (IFCTEXT)
    URL = "http://www.gortergroup.com/nl-nederlands/producten/dakluiken.html" (IFCTEXT)
    Wind- en waterdichtheid = "650 Pa" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "8mm Head" (IFCTEXT)
  Phasing | properties | on 1 object (1 IFCROOF)
    Phase Created = "New Construction" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
  Analytical Properties | properties | on 1 object (1 IFCROOF)
    Analytic Construction = "<None>" (IFCTEXT)
  Fire Protection | properties | on 1 object (1 IFCROOF)
    Brandwerendheid (aantal minuten) = 120. (IFCLENGTHMEASURE) [MILLI METRE]
    Rookdichtheid = "R 180" (IFCTEXT)
  Materials and Finishes | properties | on 1 object (1 IFCROOF)
    Hatch Material = "Gorter_Material 1" (IFCLABEL)
    Oppervlaktebehandeling binnenzijde = "Gepoedercoat RAL9010 Gepoedercoat in RAL7011 (buitenzijde) en RAL9010 (binnenzijde). Gepoedercoat RAL 9010" (IFCTEXT)
    Oppervlaktebehandeling buitenzijde = "Gepoedercoat RAL7011 Gepoedercoat in RAL7011 (buitenzijde) en RAL9010 (binnenzijde). Gepoedercoat RAL 7011" (IFCTEXT)
  Graphics | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Centre" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "M_Level Head - Circle: M_Level Head - Circle" (IFCLABEL)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)