IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "Projektnummer"
Time stamp: "2019-09-02T08:31:44"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20160225_1515(x64) - Exporter 17.0.416.0 - Alternate UI 17.12.14.0"
Application: "Autodesk Revit 2017 (ENU)" version "2017" identifier "Revit" by Organization "Autodesk Revit 2017 (ENU)"

People and organizations
  Person "Peace" of Organization (no name given)
  Owner history of Person "Peace" of Organization (no name given) | application "Autodesk Revit 2017 (ENU)" version "2017" identifier "Revit" by Organization "Autodesk Revit 2017 (ENU)" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "Projektnummer" | long name "Projektname" | phase "Projektstatus"
  IFCSITE "Default" | latitude 42° 12′ 46.804504″ | longitude -71° 2′ 0.602416″ | elevation above sea level 0.
    IFCBUILDING | postal address: "## Straße Ort, Bundesland PLZ", "Boston", "MA"
      IFCBUILDINGSTOREY "Ebene 1" | long name "Ebene 1" | elevation 0.
        contains 1 element
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "LOROWERK 00220-CC0X" | object type "LOROWERK 00220-CC0X" | names: "LOROWERK 00220-CC0X:LOROWERK 00220-CC0X:208153" | material: materials ("ConnectorOutletMediumMaterial", "ConnectorInletMediumMaterial", "Material_5070") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Constraints, Dimensions, Graphics, Insulation

Types
  IFCPIPEFITTINGTYPE "LOROWERK 00220-CC0X" | 1 occurrence | material: materials ("ConnectorOutletMediumMaterial", "ConnectorInletMediumMaterial", "Material_5070") | property sets: Data, Dimensions, General, Identity Data, Other

Property sets
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
    Client Name = "Besitzer" (IFCTEXT)
    Project Address = "## Straße Ort, Bundesland PLZ" (IFCTEXT)
    Project Issue Date = "Ausgabedatum" (IFCTEXT)
    Project Name = "Projektname" (IFCTEXT)
    Project Number = "Projektnummer" (IFCTEXT)
    Project Status = "Projektstatus" (IFCTEXT)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Other | properties | on 1 object (1 IFCFLOWFITTING)
    Category = "Pipe Fittings" (IFCLABEL)
    Family = "LOROWERK 00220-CC0X: LOROWERK 00220-CC0X" (IFCLABEL)
    Family and Type = "LOROWERK 00220-CC0X: LOROWERK 00220-CC0X" (IFCLABEL)
    Type = "LOROWERK 00220-CC0X: LOROWERK 00220-CC0X" (IFCLABEL)
    Type Id = "LOROWERK 00220-CC0X: LOROWERK 00220-CC0X" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: 8 mm Kopf" (IFCLABEL)
    Family and Type = "Level: 8 mm Kopf" (IFCLABEL)
    Type = "Level: 8 mm Kopf" (IFCLABEL)
    Type Id = "Level: 8 mm Kopf" (IFCLABEL)
  Other | properties | on 1 type object
    Category = "Pipe Fittings" (IFCLABEL)
    Family Name = "LOROWERK 00220-CC0X" (IFCTEXT)
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Author = "" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "8 mm Kopf" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Ebene 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    DATANORM = "00220.CC0X" (IFCTEXT)
    Description = "LORO-X Stahlabflussrohre" (IFCTEXT)
    GTIN = "4038088013526" (IFCTEXT)
    HAN = "00220.CC0X" (IFCTEXT)
    Manufacturer = "LOROWERK K.H. Vahlbrauk GmbH & Co. KG" (IFCTEXT)
    OmniClass Number = "" (IFCTEXT)
    OmniClass Title = "" (IFCTEXT)
    Type Name = "LORO-X Abzweig 45°" (IFCTEXT)
    VDIBSN = "020001???001001???00100100000100300700000000000130000000000000000002" (IFCTEXT)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCFLOWFITTING)
    Manufacturer = "LOROWERK K.H. Vahlbrauk GmbH & Co. KG" (IFCLABEL)
  Pset_DistributionFlowElementCommon | properties | on 1 object (1 IFCFLOWFITTING)
    Reference = "LOROWERK 00220-CC0X" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCFLOWFITTING)
    Host = "Level : Ebene 1" (IFCTEXT)
    Level = "Level: Ebene 1" (IFCLABEL)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Dimensions | properties | on 1 object (1 IFCFLOWFITTING)
    Area = 0.116737572613575 (IFCAREAMEASURE) [SQUARE_METRE]
    Maximum Size = 70. (IFCLENGTHMEASURE) [MILLI METRE]
    Minimum Size = 70. (IFCLENGTHMEASURE) [MILLI METRE]
    Size = "70 mmø-70 mmø-70 mmø" (IFCTEXT)
    Volume = 0.00475810651113787 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 type object
    CONNECTOR0_DIAMETER_dNBN0_0r = 70. (IFCLENGTHMEASURE) [MILLI METRE]
    CONNECTOR0_dNBN0_00 = 111.989597547857 (IFCLENGTHMEASURE) [MILLI METRE]
    CONNECTOR0_dNBN0_01 = 169.989597547857 (IFCLENGTHMEASURE) [MILLI METRE]
    CONNECTOR0_ref_dNBN0 = 111.989597547857 (IFCLENGTHMEASURE) [MILLI METRE]
    CONNECTOR1_DIAMETER_dX_0r = 70. (IFCLENGTHMEASURE) [MILLI METRE]
    CONNECTOR1_dX_00 = 111.989996114523 (IFCLENGTHMEASURE) [MILLI METRE]
    CONNECTOR1_dX_01 = 169.989996114523 (IFCLENGTHMEASURE) [MILLI METRE]
    CONNECTOR1_ref_dX = 111.989996114523 (IFCLENGTHMEASURE) [MILLI METRE]
    CONNECTOR2_DIAMETER_dX_0r = 70. (IFCLENGTHMEASURE) [MILLI METRE]
    CONNECTOR2_dX_00 = 85.0000093854766 (IFCLENGTHMEASURE) [MILLI METRE]
    CONNECTOR2_dX_01 = 27.0000093854766 (IFCLENGTHMEASURE) [MILLI METRE]
    CONNECTOR2_ref_dX = 27.0000093854766 (IFCLENGTHMEASURE) [MILLI METRE]
  Graphics | properties | on 1 object (1 IFCFLOWFITTING)
    Use Annotation Scale = FALSE (IFCBOOLEAN)
  Graphics | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Mitte (1)" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "M_Ebenenbeschriftung - Kreis: M_Ebenenbeschriftung - Kreis" (IFCLABEL)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Insulation | properties | on 1 object (1 IFCFLOWFITTING)
    Insulation Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Overall Size = "70 mmø-70 mmø-70 mmø" (IFCTEXT)
  Mechanical | properties | on 1 object (1 IFCFLOWFITTING)
    Loss Method = "3bf616f9-6b98-4a21-80ff-da1120c8f6d6" (IFCTEXT)
    System Abbreviation = "" (IFCTEXT)
    System Classification = "Undefined" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Phasing | properties | on 1 object (1 IFCFLOWFITTING)
    Phase Created = "Neue Konstruktion" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
  Data | properties | on 1 type object
    Formstück-Gewicht [kg] = 1.3 (IFCREAL)
    Index = 20. (IFCREAL)
    Index Number = 2. (IFCREAL)
    max. zul. Dauer-Betriebstemperatur [°C] = 95. (IFCREAL)
  General | properties | on 1 type object
    BIM = "https://media.stage.bim.site/t/eyJhbGciOiJIUzI1NiIsInR5cCI6IkpXVCJ9.eyJjdCI6MSwidGYiOiJwdWJsaWMvbG9yb3dlcmsta2gtdmFobGJyYXVrLWdtYmgtY28ta2cvZjVhMjlmMS9QQVJUMjlfTG9yb18yMDE5MDcwMV8xLlZESSIsImNpZCI6IjMyNzdjYzIzLTgxYTktNGVlMy1hOTBhLWI0N2JiNGMwYjYxNiIsInJpZCI6IjFlZGU5MWM4MTFmYzhiMTYwYjcxZjBmMDZhOTFjODM0IiwicGlkIjoiNDI4YTAwZGFmZWQxZDA4NjE2YjAxZGM1Y2IxZGVhZDkzYTJiOGFjYSIsInNpZCI6IjY2MzI1IiwidXQiOjUsImxjIjoiZGUiLCJpYXQiOjE1NjczMDk4MDcsImlzcyI6Imh0dHBzOi8vYXBpLmxpdmUuYmltLnNpdGUiLCJzdWIiOiJyZXZpdC50ZWFtMjRAZ21haWwuY29tIn0.hskWNtjCz7AJZOeQ4RYoftsbM5iUmNvgZbZXKi0-v9c/PART29_Loro_20190701_1.VDI" (IFCTEXT)
    Benennung = "LORO-X Abzweig 45°, DN70/70" (IFCTEXT)
    Brandschutzklasse = "B1 nach DIN 4102" (IFCTEXT)
    HeinzeBIM = "https://www.heinze.de/bim/loro-x-abzweig-45-/428a00dafed1d08616b01dc5cb1dead93a2b8aca" (IFCTEXT)
    Nenndruck = "0.5" (IFCTEXT)
    Nenndrucksystem = "PN" (IFCTEXT)
    Nennweitensystem = "DN" (IFCTEXT)
    Normen/Regeln/Zulassungen = "DVGW für Trinkwasser" (IFCTEXT)
    Produktbezeichnung = "Entsorgung" (IFCTEXT)
    Produktbezeichnung Text = "LORO-X Stahlabflussrohre" (IFCTEXT)
    Produktkennung = "Formstück" (IFCTEXT)
    Produktname = "LORO-X Abzweig 45°" (IFCTEXT)
    Produktvideo = "https://media.stage.bim.site/t/eyJhbGciOiJIUzI1NiIsInR5cCI6IkpXVCJ9.eyJjdCI6MiwidHUiOiJodHRwOi8vd3d3Lmxvcm8uZGUvaW5kZXgucGhwP2lkPTIzM1x1MDAyNmFydGlrZWxucj0wMDIyMC5DQzBYIiwiY2lkIjoiMzI3N2NjMjMtODFhOS00ZWUzLWE5MGEtYjQ3YmI0YzBiNjE2IiwicmlkIjoiMWVkZTkxYzgxMWZjOGIxNjBiNzFmMGYwNmE5MWM4MzQiLCJwaWQiOiI0MjhhMDBkYWZlZDFkMDg2MTZiMDFkYzVjYjFkZWFkOTNhMmI4YWNhIiwic2lkIjoiNjYzMjUiLCJ1dCI6MiwibGMiOiJkZSIsImlhdCI6MTU2NzMwOTgwNywiaXNzIjoiaHR0cHM6Ly9hcGkubGl2ZS5iaW0uc2l0ZSIsInN1YiI6InJldml0LnRlYW0yNEBnbWFpbC5jb20ifQ.LQNx_Ea3ixT-Z9UamxMM6yJVwwl2bUWZFe08I6gwCK4" (IFCTEXT)
    Querschnittsform = "rund" (IFCTEXT)
    Verbindungsart I = "Pressen" (IFCTEXT)
    Verbindungsart II = "axial pressen" (IFCTEXT)
    Verlegeart = "Unterputz" (IFCTEXT)