IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition[CoordinationView]"
Time stamp: "2021-11-17T16:56:41"
Author: "NBS"
Preprocessor: "Xbim.Ifc File Processor version 2.4.1.0"
Originating system: "Xbim version 2.4.1.0"
Authorization: "Add company name here"
Application: "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS"

People and organizations
  Person "NBS" of Organization "Add company name here"
  Owner history of Person "NBS" of Organization "Add company name here" | application "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS" | change ADDED | created 1637168202 (2021-11-17T16:56:42Z)
  Owner history of Person "NBS" of Organization "Add company name here" | application "Add company name here" version "0.2" identifier "Xbim Layered Material Converter" by Organization "NBS" | change MODIFIED | created 1637168202 (2021-11-17T16:56:42Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  SOLIDANGLEUNIT: STERADIAN
  PLANEANGLEUNIT: RADIAN
  MASSUNIT: GRAM
  TIMEUNIT: SECOND
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  LUMINOUSINTENSITYUNIT: LUMEN

Spatial structure
IFCPROJECT "Add company name here"
  IFCSITE "Default site"
    IFCBUILDING "Default building"
      contains 7 elements
        1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "NBS_wediSystemsUKLtd_ExtrudedPolystyreneBoard_wediBuildingBoardVapor_2500x600x14mm" | names: "NBS_wediSystemsUKLtd_ExtrudedPolystyreneBoard_wediBuildingBoardVapor_2500x600x14mm" | material: layers "NBS_wediSystemsUKLtd_ExtrudedPolystyreneBoard_wediBuildingBoardVapor_2500x600x14mm" ("NBS_wediSystemsUKLtd_ExtrudedPolystyreneBoard_wediBuildingBoardVapor_2500x600x14mm" 14.) | property sets: COBie
        1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "NBS_wediSystemsUKLtd_ExtrudedPolystyreneBoard_wediBuildingBoardVapor_2500x600x21.5mm" | names: "NBS_wediSystemsUKLtd_ExtrudedPolystyreneBoard_wediBuildingBoardVapor_2500x600x21.5mm" | material: layers "NBS_wediSystemsUKLtd_ExtrudedPolystyreneBoard_wediBuildingBoardVapor_2500x600x21.5mm" ("NBS_wediSystemsUKLtd_ExtrudedPolystyreneBoard_wediBuildingBoardVapor_2500x600x21.5mm" 21.5) | property sets: COBie
        1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "NBS_wediSystemsUKLtd_ExtrudedPolystyreneBoard_wediBuildingBoardVapor_2500x600x51.5mm" | names: "NBS_wediSystemsUKLtd_ExtrudedPolystyreneBoard_wediBuildingBoardVapor_2500x600x51.5mm" | material: layers "NBS_wediSystemsUKLtd_ExtrudedPolystyreneBoard_wediBuildingBoardVapor_2500x600x51.5mm" ("NBS_wediSystemsUKLtd_ExtrudedPolystyreneBoard_wediBuildingBoardVapor_2500x600x51.5mm" 51.5) | property sets: COBie
        1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "NBS_wediSystemsUKLtd_ExtrudedPolystyreneBoard_wediBuildingBoardVapor85_2500x600x12.5mm" | names: "NBS_wediSystemsUKLtd_ExtrudedPolystyreneBoard_wediBuildingBoardVapor85_2500x600x12.5mm" | material: layers "NBS_wediSystemsUKLtd_ExtrudedPolystyreneBoard_wediBuildingBoardVapor85_2500x600x12.5mm" ("NBS_wediSystemsUKLtd_ExtrudedPolystyreneBoard_wediBuildingBoardVapor85_2500x600x12.5mm" 12.5) | property sets: COBie
        1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "NBS_wediSystemsUKLtd_ExtrudedPolystyreneBoard_wediBuildingBoardVapor85_2500x600x20mm" | names: "NBS_wediSystemsUKLtd_ExtrudedPolystyreneBoard_wediBuildingBoardVapor85_2500x600x20mm" | material: layers "NBS_wediSystemsUKLtd_ExtrudedPolystyreneBoard_wediBuildingBoardVapor85_2500x600x20mm" ("NBS_wediSystemsUKLtd_ExtrudedPolystyreneBoard_wediBuildingBoardVapor85_2500x600x20mm" 20.) | property sets: COBie
        1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "NBS_wediSystemsUKLtd_ExtrudedPolystyreneBoard_wediBuildingBoardVapor85_2500x900x12.5mm" | names: "NBS_wediSystemsUKLtd_ExtrudedPolystyreneBoard_wediBuildingBoardVapor85_2500x900x12.5mm" | material: layers "NBS_wediSystemsUKLtd_ExtrudedPolystyreneBoard_wediBuildingBoardVapor85_2500x900x12.5mm" ("NBS_wediSystemsUKLtd_ExtrudedPolystyreneBoard_wediBuildingBoardVapor85_2500x900x12.5mm" 12.5) | property sets: COBie
        1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "NBS_wediSystemsUKLtd_ExtrudedPolystyreneBoard_wediBuildingBoardVapor85_2500x900x20mm" | names: "NBS_wediSystemsUKLtd_ExtrudedPolystyreneBoard_wediBuildingBoardVapor85_2500x900x20mm" | material: layers "NBS_wediSystemsUKLtd_ExtrudedPolystyreneBoard_wediBuildingBoardVapor85_2500x900x20mm" ("NBS_wediSystemsUKLtd_ExtrudedPolystyreneBoard_wediBuildingBoardVapor85_2500x900x20mm" 20.) | property sets: COBie

Types
  IFCWALLTYPE "NBS_wediSystemsUKLtd_ExtrudedPolystyreneBoard_wediBuildingBoardVapor_2500x600x14mm" | STANDARD | 1 occurrence | material: layers "NBS_wediSystemsUKLtd_ExtrudedPolystyreneBoard_wediBuildingBoardVapor_2500x600x14mm" ("NBS_wediSystemsUKLtd_ExtrudedPolystyreneBoard_wediBuildingBoardVapor_2500x600x14mm" 14.) | property sets: xbim_MaterialFunctionAssignment, COBie, Pset_CoveringCommon, BOS_General, NBS_Data
  IFCWALLTYPE "NBS_wediSystemsUKLtd_ExtrudedPolystyreneBoard_wediBuildingBoardVapor_2500x600x21.5mm" | STANDARD | 1 occurrence | material: layers "NBS_wediSystemsUKLtd_ExtrudedPolystyreneBoard_wediBuildingBoardVapor_2500x600x21.5mm" ("NBS_wediSystemsUKLtd_ExtrudedPolystyreneBoard_wediBuildingBoardVapor_2500x600x21.5mm" 21.5) | property sets: xbim_MaterialFunctionAssignment, COBie, Pset_CoveringCommon, BOS_General, NBS_Data
  IFCWALLTYPE "NBS_wediSystemsUKLtd_ExtrudedPolystyreneBoard_wediBuildingBoardVapor_2500x600x51.5mm" | STANDARD | 1 occurrence | material: layers "NBS_wediSystemsUKLtd_ExtrudedPolystyreneBoard_wediBuildingBoardVapor_2500x600x51.5mm" ("NBS_wediSystemsUKLtd_ExtrudedPolystyreneBoard_wediBuildingBoardVapor_2500x600x51.5mm" 51.5) | property sets: xbim_MaterialFunctionAssignment, COBie, Pset_CoveringCommon, BOS_General, NBS_Data
  IFCWALLTYPE "NBS_wediSystemsUKLtd_ExtrudedPolystyreneBoard_wediBuildingBoardVapor85_2500x600x12.5mm" | STANDARD | 1 occurrence | material: layers "NBS_wediSystemsUKLtd_ExtrudedPolystyreneBoard_wediBuildingBoardVapor85_2500x600x12.5mm" ("NBS_wediSystemsUKLtd_ExtrudedPolystyreneBoard_wediBuildingBoardVapor85_2500x600x12.5mm" 12.5) | property sets: xbim_MaterialFunctionAssignment, COBie, Pset_CoveringCommon, BOS_General, NBS_Data
  IFCWALLTYPE "NBS_wediSystemsUKLtd_ExtrudedPolystyreneBoard_wediBuildingBoardVapor85_2500x600x20mm" | STANDARD | 1 occurrence | material: layers "NBS_wediSystemsUKLtd_ExtrudedPolystyreneBoard_wediBuildingBoardVapor85_2500x600x20mm" ("NBS_wediSystemsUKLtd_ExtrudedPolystyreneBoard_wediBuildingBoardVapor85_2500x600x20mm" 20.) | property sets: xbim_MaterialFunctionAssignment, COBie, Pset_CoveringCommon, BOS_General, NBS_Data
  IFCWALLTYPE "NBS_wediSystemsUKLtd_ExtrudedPolystyreneBoard_wediBuildingBoardVapor85_2500x900x12.5mm" | STANDARD | 1 occurrence | material: layers "NBS_wediSystemsUKLtd_ExtrudedPolystyreneBoard_wediBuildingBoardVapor85_2500x900x12.5mm" ("NBS_wediSystemsUKLtd_ExtrudedPolystyreneBoard_wediBuildingBoardVapor85_2500x900x12.5mm" 12.5) | property sets: xbim_MaterialFunctionAssignment, COBie, Pset_CoveringCommon, BOS_General, NBS_Data
  IFCWALLTYPE "NBS_wediSystemsUKLtd_ExtrudedPolystyreneBoard_wediBuildingBoardVapor85_2500x900x20mm" | STANDARD | 1 occurrence | material: layers "NBS_wediSystemsUKLtd_ExtrudedPolystyreneBoard_wediBuildingBoardVapor85_2500x900x20mm" ("NBS_wediSystemsUKLtd_ExtrudedPolystyreneBoard_wediBuildingBoardVapor85_2500x900x20mm" 20.) | property sets: xbim_MaterialFunctionAssignment, COBie, Pset_CoveringCommon, BOS_General, NBS_Data

Property sets
  COBie | properties | on 7 objects (7 IFCWALLSTANDARDCASE)
    AssetIdentifier = "n/a" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Pr_25_71_63_29:Extruded polystyrene (XPS) boards" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "Grey" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "wedi building board Vapor 14mm" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "30" (IFCTEXT)
    Features = "For walls, ceilings and floors, waterproof and heat-insulating" (IFCTEXT)
    Finish = "Resistant and glass fibre reinforced cement coating" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Manufacturer = "technical@wedi.co.uk" (IFCTEXT)
    Material = "A waterproof extruded polystyrene rigid foam core with a special, resistant and glass fibre reinforced cement coating, with a vapour barrier on one side" (IFCTEXT)
    ModelNumber = "010713112" (IFCTEXT)
    ModelReference = "wedi building board Vapor" (IFCTEXT)
    Name = "ExtrudedPolystyreneBoard_wediBuildingBoardVapor_2500x600x14mm_wediSystemsLtd" (IFCTEXT)
    NominalHeight = 14. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 2500. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 600. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "Rectangle" (IFCTEXT)
    Size = "2500 x 600 x 14 mm" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "Available on request" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Pr_25_71_63_29:Extruded polystyrene (XPS) boards" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "Grey" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "wedi building board Vapor 21,5mm" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "30" (IFCTEXT)
    Features = "For walls, ceilings and floors, waterproof and heat-insulating" (IFCTEXT)
    Finish = "Resistant and glass fibre reinforced cement coating" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Manufacturer = "technical@wedi.co.uk" (IFCTEXT)
    Material = "A waterproof extruded polystyrene rigid foam core with a special, resistant and glass fibre reinforced cement coating, with a vapour barrier on one side" (IFCTEXT)
    ModelNumber = "010713020" (IFCTEXT)
    ModelReference = "wedi building board Vapor" (IFCTEXT)
    Name = "ExtrudedPolystyreneBoard_wediBuildingBoardVapor_2500x600x21.5mm_wediSystemsLtd" (IFCTEXT)
    NominalHeight = 21.5 (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 2500. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 600. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "Rectangle" (IFCTEXT)
    Size = "2500 x 600 x 21.5 mm" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "Available on request" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Pr_25_71_63_29:Extruded polystyrene (XPS) boards" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "Grey" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "wedi building board Vapor 51,5mm" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "30" (IFCTEXT)
    Features = "For walls, ceilings and floors, waterproof and heat-insulating" (IFCTEXT)
    Finish = "Resistant and glass fibre reinforced cement coating" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Manufacturer = "technical@wedi.co.uk" (IFCTEXT)
    Material = "A waterproof extruded polystyrene rigid foam core with a special, resistant and glass fibre reinforced cement coating, with a vapour barrier on one side" (IFCTEXT)
    ModelNumber = "010713050" (IFCTEXT)
    ModelReference = "wedi building board Vapor" (IFCTEXT)
    Name = "ExtrudedPolystyreneBoard_wediBuildingBoardVapor_2500x600x21.5mm_wediSystemsLtd" (IFCTEXT)
    NominalHeight = 51.5 (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 2500. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 600. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "Rectangle" (IFCTEXT)
    Size = "2500 x 600 x 51.5 mm" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "Available on request" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Pr_25_71_63_29:Extruded polystyrene (XPS) boards" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "Grey" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "wedi building board Vapor 85 12,5mm" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "30" (IFCTEXT)
    Features = "For walls, ceilings and floors, waterproof and heat-insulating" (IFCTEXT)
    Finish = "Resistant and glass fibre reinforced cement coating" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Manufacturer = "technical@wedi.co.uk" (IFCTEXT)
    Material = "A waterproof extruded polystyrene rigid foam core with a special, resistant and glass fibre reinforced cement coating, with a pre-integrated vapour membrane" (IFCTEXT)
    ModelNumber = "010702012" (IFCTEXT)
    ModelReference = "wedi building board Vapor 85" (IFCTEXT)
    Name = "ExtrudedPolystyreneBoard_wediBuildingBoardVapor85_2500x600x12.5mm_wediSystemsLtd" (IFCTEXT)
    NominalHeight = 12.5 (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 2500. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 600. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "Rectangle" (IFCTEXT)
    Size = "2500 x 600 x 12.5 mm" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "Available on request" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Pr_25_71_63_29:Extruded polystyrene (XPS) boards" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "Grey" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "wedi building board Vapor 85 20mm" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "30" (IFCTEXT)
    Features = "For walls, ceilings and floors, waterproof and heat-insulating" (IFCTEXT)
    Finish = "Resistant and glass fibre reinforced cement coating" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Manufacturer = "technical@wedi.co.uk" (IFCTEXT)
    Material = "A waterproof extruded polystyrene rigid foam core with a special, resistant and glass fibre reinforced cement coating, with a pre-integrated vapour membrane" (IFCTEXT)
    ModelNumber = "010702020" (IFCTEXT)
    ModelReference = "wedi Vapor85 building board" (IFCTEXT)
    Name = "ExtrudedPolystyreneBoard_wediBuildingBoardVapor85_2500x600x20mm_wediSystemsLtd" (IFCTEXT)
    NominalHeight = 20. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 2500. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 600. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "Rectangle" (IFCTEXT)
    Size = "2500 x 600 x 20 mm" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "Available on request" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Pr_25_71_63_29:Extruded polystyrene (XPS) boards" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "Grey" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "wedi building board Vapor 85 12,5mm" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "30" (IFCTEXT)
    Features = "For walls, ceilings and floors, waterproof and heat-insulating" (IFCTEXT)
    Finish = "Resistant and glass fibre reinforced cement coating" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Manufacturer = "technical@wedi.co.uk" (IFCTEXT)
    Material = "A waterproof extruded polystyrene rigid foam core with a special, resistant and glass fibre reinforced cement coating, with a pre-integrated vapour membrane" (IFCTEXT)
    ModelNumber = "010702912" (IFCTEXT)
    ModelReference = "wedi Vapor85 building board" (IFCTEXT)
    Name = "ExtrudedPolystyreneBoard_wediBuildingBoardVapor85_2500x900x12.5mm_wediSystemsLtd" (IFCTEXT)
    NominalHeight = 12.5 (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 2500. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 900. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "Rectangle" (IFCTEXT)
    Size = "2500 x 900 x 12.5 mm" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "Available on request" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Pr_25_71_63_29:Extruded polystyrene (XPS) boards" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "Grey" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "wedi building board Vapor 85 20mm" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "30" (IFCTEXT)
    Features = "For walls, ceilings and floors, waterproof and heat-insulating" (IFCTEXT)
    Finish = "Resistant and glass fibre reinforced cement coating" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Manufacturer = "technical@wedi.co.uk" (IFCTEXT)
    Material = "A waterproof extruded polystyrene rigid foam core with a special, resistant and glass fibre reinforced cement coating, with a pre-integrated vapour membrane" (IFCTEXT)
    ModelNumber = "010702920" (IFCTEXT)
    ModelReference = "wedi Vapor85 building board" (IFCTEXT)
    Name = "ExtrudedPolystyreneBoard_wediBuildingBoardVapor85_2500x900x20mm_wediSystemsLtd" (IFCTEXT)
    NominalHeight = 20. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 2500. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 900. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "Rectangle" (IFCTEXT)
    Size = "2500 x 900 x 20 mm" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "Available on request" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  xbim_MaterialFunctionAssignment | properties | on 7 type objects
    MaterialFunctionAssignment (ifcpropertytablevalue)
  Pset_CoveringCommon | properties | on 7 type objects
    AcousticRating = "23 dB" (IFCTEXT)
    Combustible = TRUE (IFCBOOLEAN)
    FireRating = "Class E" (IFCTEXT)
    FlammabilityRating = "n/a" (IFCTEXT)
    FragilityRating = "n/a" (IFCTEXT)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "n/a" (IFCTEXT)
    Status = "UNSET" (IFCTEXT)
    SurfaceSpreadOfFlame = "n/a" (IFCTEXT)
    ThermalTransmittance = 0. (IFCREAL)
  BOS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_wediSystemsUKLtd_ExtrudedPolystyreneBoard_wediBuildingBoardVapor_2500x600x14mm" (IFCTEXT)
    ManufacturerName = "wedi Systems (UK) Ltd" (IFCTEXT)
    ManufacturerURL = "https://www.wedi.de/uk/" (IFCTEXT)
    NBSCertification = "www.nationalbimlibrary.com/cert/1ntcymfb" (IFCTEXT)
    NBSDescription = "Extruded polystyrene (XPS) board" (IFCTEXT)
    NBSReference = "45-45-65/410" (IFCTEXT)
    ProductInformation = "https://www.wedi.de/en/products/building-systems/building-board/building-board-vapor/" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2015Code = "Pr_25_71_63_29" (IFCTEXT)
    Uniclass2015Title = "Extruded polystyrene (XPS) boards" (IFCTEXT)
    Uniclass2015Version = "Products v1.14" (IFCTEXT)
    Version = "1" (IFCTEXT)
  BOS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_wediSystemsUKLtd_ExtrudedPolystyreneBoard_wediBuildingBoardVapor_2500x600x21.5mm" (IFCTEXT)
    ManufacturerName = "wedi Systems (UK) Ltd" (IFCTEXT)
    ManufacturerURL = "https://www.wedi.de/uk/" (IFCTEXT)
    NBSCertification = "www.nationalbimlibrary.com/cert/1ntcymfb" (IFCTEXT)
    NBSDescription = "Extruded polystyrene (XPS) board" (IFCTEXT)
    NBSReference = "45-45-65/410" (IFCTEXT)
    ProductInformation = "https://www.wedi.de/en/products/building-systems/building-board/building-board-vapor/" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2015Code = "Pr_25_71_63_29" (IFCTEXT)
    Uniclass2015Title = "Extruded polystyrene (XPS) boards" (IFCTEXT)
    Uniclass2015Version = "Products v1.14" (IFCTEXT)
    Version = "1" (IFCTEXT)
  BOS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_wediSystemsUKLtd_ExtrudedPolystyreneBoard_wediBuildingBoardVapor_2500x600x51.5mm" (IFCTEXT)
    ManufacturerName = "wedi Systems (UK) Ltd" (IFCTEXT)
    ManufacturerURL = "https://www.wedi.de/uk/" (IFCTEXT)
    NBSCertification = "www.nationalbimlibrary.com/cert/1ntcymfb" (IFCTEXT)
    NBSDescription = "Extruded polystyrene (XPS) board" (IFCTEXT)
    NBSReference = "45-45-65/410" (IFCTEXT)
    ProductInformation = "https://www.wedi.de/en/products/building-systems/building-board/building-board-vapor/" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2015Code = "Pr_25_71_63_29" (IFCTEXT)
    Uniclass2015Title = "Extruded polystyrene (XPS) boards" (IFCTEXT)
    Uniclass2015Version = "Products v1.14" (IFCTEXT)
    Version = "1" (IFCTEXT)
  BOS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_wediSystemsUKLtd_ExtrudedPolystyreneBoard_wediBuildingBoardVapor85_2500x600x12.5mm" (IFCTEXT)
    ManufacturerName = "wedi Systems (UK) Ltd" (IFCTEXT)
    ManufacturerURL = "https://www.wedi.de/uk/" (IFCTEXT)
    NBSCertification = "www.nationalbimlibrary.com/cert/1ntcymfb" (IFCTEXT)
    NBSDescription = "Extruded polystyrene (XPS) board" (IFCTEXT)
    NBSReference = "45-45-65/410" (IFCTEXT)
    ProductInformation = "https://www.wedi.de/en/products/building-systems/building-board/wedi-vapor-85/" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2015Code = "Pr_25_71_63_29" (IFCTEXT)
    Uniclass2015Title = "Extruded polystyrene (XPS) boards" (IFCTEXT)
    Uniclass2015Version = "Products v1.14" (IFCTEXT)
    Version = "1" (IFCTEXT)
  BOS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_wediSystemsUKLtd_ExtrudedPolystyreneBoard_wediBuildingBoardVapor85_2500x600x20mm" (IFCTEXT)
    ManufacturerName = "wedi Systems (UK) Ltd" (IFCTEXT)
    ManufacturerURL = "https://www.wedi.de/uk/" (IFCTEXT)
    NBSCertification = "www.nationalbimlibrary.com/cert/1ntcymfb" (IFCTEXT)
    NBSDescription = "Extruded polystyrene (XPS) board" (IFCTEXT)
    NBSReference = "45-45-65/410" (IFCTEXT)
    ProductInformation = "https://www.wedi.de/en/products/building-systems/building-board/wedi-vapor-85/" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2015Code = "Pr_25_71_63_29" (IFCTEXT)
    Uniclass2015Title = "Extruded polystyrene (XPS) boards" (IFCTEXT)
    Uniclass2015Version = "Products v1.14" (IFCTEXT)
    Version = "1" (IFCTEXT)
  BOS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_wediSystemsUKLtd_ExtrudedPolystyreneBoard_wediBuildingBoardVapor85_2500x900x12.5mm" (IFCTEXT)
    ManufacturerName = "wedi Systems (UK) Ltd" (IFCTEXT)
    ManufacturerURL = "https://www.wedi.de/uk/" (IFCTEXT)
    NBSCertification = "www.nationalbimlibrary.com/cert/1ntcymfb" (IFCTEXT)
    NBSDescription = "Extruded polystyrene (XPS) board" (IFCTEXT)
    NBSReference = "45-45-65/410" (IFCTEXT)
    ProductInformation = "https://www.wedi.de/en/products/building-systems/building-board/wedi-vapor-85/" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2015Code = "Pr_25_71_63_29" (IFCTEXT)
    Uniclass2015Title = "Extruded polystyrene (XPS) boards" (IFCTEXT)
    Uniclass2015Version = "Products v1.14" (IFCTEXT)
    Version = "1" (IFCTEXT)
  BOS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_wediSystemsUKLtd_ExtrudedPolystyreneBoard_wediBuildingBoardVapor85_2500x900x20mm" (IFCTEXT)
    ManufacturerName = "wedi Systems (UK) Ltd" (IFCTEXT)
    ManufacturerURL = "https://www.wedi.de/uk/" (IFCTEXT)
    NBSCertification = "www.nationalbimlibrary.com/cert/1ntcymfb" (IFCTEXT)
    NBSDescription = "Extruded polystyrene (XPS) board" (IFCTEXT)
    NBSReference = "45-45-65/410" (IFCTEXT)
    ProductInformation = "https://www.wedi.de/en/products/building-systems/building-board/wedi-vapor-85/" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2015Code = "Pr_25_71_63_29" (IFCTEXT)
    Uniclass2015Title = "Extruded polystyrene (XPS) boards" (IFCTEXT)
    Uniclass2015Version = "Products v1.14" (IFCTEXT)
    Version = "1" (IFCTEXT)
  NBS_Data | properties | on 4 type objects
    CompressiveStrength = "0.08 N/mm²" (IFCTEXT)
    Edges = "n/a" (IFCTEXT)
    Elasticity = "10 – 18 N/mm²" (IFCTEXT)
    Facing = "With pre-installed vapour barrier" (IFCTEXT)
    RecycledContent = "n/a" (IFCTEXT)
    ShearModulusValue = "7 N/mm²" (IFCTEXT)
    TensileStrength = "0.45 N/mm²" (IFCTEXT)
    ThermalConductivity = "0.036 W/mK" (IFCTEXT)
    WaterAbsorption = "≤1.5 Vol.-%" (IFCTEXT)
  NBS_Data | properties | on 3 type objects
    CompressiveStrength = "0.08 N/mm²" (IFCTEXT)
    Edges = "n/a" (IFCTEXT)
    Elasticity = "10 – 18 N/mm²" (IFCTEXT)
    Facing = "With epoxy vapour barrier" (IFCTEXT)
    RecycledContent = "n/a" (IFCTEXT)
    ShearModulusValue = "7 N/mm²" (IFCTEXT)
    TensileStrength = "0.45 N/mm²" (IFCTEXT)
    ThermalConductivity = "0.036 W/mK" (IFCTEXT)
    WaterAbsorption = "≤1.5 Vol.-%" (IFCTEXT)