IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "Project Number"
Time stamp: "2020-01-15T14:21:37"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20190808_0900(x64) - Exporter 19.2.20.24 - IFC Model Exchange with ARCHICAD 22.0.0.6010"
Application: "Autodesk Revit 2019 (ENU)" version "2019" identifier "Revit" by Organization "Autodesk Revit 2019 (ENU)"

People and organizations
  Person "sebastian.walicki" of Organization (no name given)
  Owner history of Person "sebastian.walicki" of Organization (no name given) | application "Autodesk Revit 2019 (ENU)" version "2019" identifier "Revit" by Organization "Autodesk Revit 2019 (ENU)" | change NOCHANGE | created 1579094497 (2020-01-15T13:21:37Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 21′ 31.181945″ | longitude -71° 3′ 24.263305″ | elevation above sea level 0.
    IFCBUILDING | postal address: "## Street City, State Zip", "Boston", "MA"
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | elevation 0.
        contains 1 element
          1 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "92583 - pd11-m-1c-flat-fc - recessed ceiling mounted_beg_dixh 52x60 mm" | object type "92583 - pd11-m-1c-flat-fc - recessed ceiling mounted_beg_dixh 52x60 mm" | names: "RSen_62_LD_FB_movement sensor - 1 channel_beg:92583 - pd11-m-1c-flat-fc - recessed ceiling mounted_beg_dixh 52x60 mm:294053" | material: materials ("RSen_rgb_241_236_225_T00 RAL9010_gen", "Glass") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Constraints, Construction, Dimensions, Electrical

Types
  IFCAIRTERMINALTYPE "92583 - pd11-m-1c-flat-fc - recessed ceiling mounted_beg_dixh 52x60 mm" | 1 occurrence | material: materials ("RSen_rgb_241_236_225_T00 RAL9010_gen", "Glass") | property sets: Constraints, Construction, Dimensions, Electrical, Identity Data, Materials and Finishes

Property sets
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "8mm Head" (IFCTEXT)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCFLOWTERMINAL)
    Manufacturer = "BEG" (IFCLABEL)
  Pset_DistributionFlowElementCommon | properties | on 1 object (1 IFCFLOWTERMINAL)
    Reference = "RSen_62_LD_FB_movement sensor - 1 channel_beg:92583 - pd11-m-1c-flat-fc - recessed ceiling mounted_beg_dixh 52x60 mm" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCFLOWTERMINAL)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "Reference Plane : h_leftright" (IFCTEXT)
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 type object
    Default Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Construction | properties | on 1 object (1 IFCFLOWTERMINAL)
    RSen_C_accessory_EE_01 = "none_gen" (IFCLABEL)
    RSen_C_alignment = "Center" (IFCTEXT)
    RSen_C_alignment_index = 0 (IFCINTEGER)
    RSen_C_mounting_elevation = 2500. (IFCLENGTHMEASURE) [MILLI METRE]
    TBQen_C_GOg = FALSE (IFCBOOLEAN)
    TBQen_C_SOg = TRUE (IFCBOOLEAN)
  Construction | properties | on 1 type object
    RSen_C_accessory_EE_02 = "none_gen" (IFCLABEL)
    RSen_C_accessory_EE_03 = "none_gen" (IFCLABEL)
    RSen_C_accessory_EE_04 = "none_gen" (IFCLABEL)
    RSen_C_accessory_EE_05 = "none_gen" (IFCLABEL)
    TBQen_C_SOg_LD_2D = "none" (IFCLABEL)
    TBQen_C_SOg_LD_3D = "standard" (IFCLABEL)
  Dimensions | properties | on 1 object (1 IFCFLOWTERMINAL)
    Area = 0.266390659025447 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.00190123626824522 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 type object
    RSen_C_diameter = 52. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_C_height = 60. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_C_length = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_C_width = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Electrical | properties | on 1 object (1 IFCFLOWTERMINAL)
    RSen_E_c01_load_class = "Lighting" (IFCLABEL)
    RSen_E_c01_power_factor = 1. (IFCREAL)
    RSen_E_knx_operation_01 = "" (IFCTEXT)
    RSen_E_knx_operation_02 = "" (IFCTEXT)
    RSen_E_knx_operation_03 = "" (IFCTEXT)
    RSen_E_knx_operation_04 = "" (IFCTEXT)
    RSen_E_knx_operation_05 = "" (IFCTEXT)
    RSen_E_knx_operation_06 = "" (IFCTEXT)
    RSen_E_power_factor = 1. (IFCREAL)
  Electrical | properties | on 1 type object
    RSen_E_c01_apparent_power = 1150. (IFCPOWERMEASURE) [WATT]
    RSen_E_c01_division_engine = FALSE (IFCBOOLEAN)
    RSen_E_c01_number_of_poles = 1 (IFCINTEGER)
    RSen_E_c01_voltage = 230. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
  Electrical - Circuiting | properties | on 1 object (1 IFCFLOWTERMINAL)
    Electrical Data = "c01_electrical connector 230 V/1-1150 VA" (IFCTEXT)
  Electrical - Loads | properties | on 1 object (1 IFCFLOWTERMINAL)
    Circuit Number = "" (IFCTEXT)
    Panel = "" (IFCTEXT)
  Graphics | properties | on 1 object (1 IFCFLOWTERMINAL)
    RSen_C_clearance_zone = FALSE (IFCBOOLEAN)
    RSen_C_detection_zone_01 = FALSE (IFCBOOLEAN)
    RSen_C_detection_zone_02 = FALSE (IFCBOOLEAN)
    RSen_C_detection_zone_03 = FALSE (IFCBOOLEAN)
    TBQen_C_logo = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Author = "" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCFLOWTERMINAL)
    Mark = "34" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "62.60.10" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Description = "RECESSED CEILING MOUNTED" (IFCTEXT)
    Manufacturer = "BEG" (IFCTEXT)
    Model = "PD11-M-1C-FLAT-FC" (IFCTEXT)
    OmniClass Number = "" (IFCTEXT)
    OmniClass Title = "" (IFCTEXT)
    RSen_C_IFC_version = "2x3" (IFCTEXT)
    RSen_C_accessory = "-" (IFCTEXT)
    RSen_C_code_ETIM = "" (IFCTEXT)
    RSen_C_code_ETIM_URL = "http://prod.etim-international.com/" (IFCTEXT)
    RSen_C_code_article = "92583" (IFCTEXT)
    RSen_C_code_gtin = "4,01E+12" (IFCTEXT)
    RSen_C_code_product = "92583" (IFCTEXT)
    RSen_C_code_product_class = "PD11-M-1C-FLAT-FC" (IFCTEXT)
    RSen_C_content_creator = "© ThorbiQ" (IFCTEXT)
    RSen_C_content_date_changed = "00/00/0000" (IFCTEXT)
    RSen_C_content_date_issue = "00/00/0000" (IFCTEXT)
    RSen_C_content_provider = "BEG" (IFCTEXT)
    RSen_C_content_version = "1.0.0" (IFCTEXT)
    RSen_C_data_issue_date = "" (IFCTEXT)
    RSen_C_description = "RECESSED CEILING MOUNTED" (IFCTEXT)
    RSen_C_license = "Creative Commons Attribution NoDerivs (CC-ND)" (IFCTEXT)
    RSen_C_license_info = "https://tldrlegal.com/license/creative-commons-attribution-noderivs-(cc-nd)#summary" (IFCTEXT)
    RSen_C_model = "PD11-M-1C-FLAT-FC" (IFCTEXT)
    RSen_C_revit_version = "2017" (IFCTEXT)
    RSen_C_type = "PD11-M-1C-FLAT-FC" (IFCTEXT)
    RSen_C_type_comments = "movement sensor" (IFCTEXT)
    TBQ_I BaseKeynote = "62.60.10" (IFCTEXT)
    Type Name = "92583 - pd11-m-1c-flat-fc - recessed ceiling mounted_beg_dixh 52x60 mm" (IFCTEXT)
    URL = "https://www.beg-luxomat.com/en/products/luxomat/ceiling-mounted-occupancy-detectors/1-channel/pd11-m-1c-flat/" (IFCTEXT)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
    Client Name = "Owner" (IFCTEXT)
    Project Address = "## Street City, State Zip" (IFCTEXT)
    Project Issue Date = "Issue Date" (IFCTEXT)
    Project Name = "Project Name" (IFCTEXT)
    Project Number = "Project Number" (IFCTEXT)
    Project Status = "Project Status" (IFCTEXT)
  Other | properties | on 1 object (1 IFCFLOWTERMINAL)
    Category = "Lighting Devices" (IFCLABEL)
    Family = "RSen_62_LD_FB_movement sensor - 1 channel_beg: 92583 - pd11-m-1c-flat-fc - recessed ceiling mounted_beg_dixh 52x60 mm" (IFCLABEL)
    Family and Type = "RSen_62_LD_FB_movement sensor - 1 channel_beg: 92583 - pd11-m-1c-flat-fc - recessed ceiling mounted_beg_dixh 52x60 mm" (IFCLABEL)
    Type = "RSen_62_LD_FB_movement sensor - 1 channel_beg: 92583 - pd11-m-1c-flat-fc - recessed ceiling mounted_beg_dixh 52x60 mm" (IFCLABEL)
    Type Id = "RSen_62_LD_FB_movement sensor - 1 channel_beg: 92583 - pd11-m-1c-flat-fc - recessed ceiling mounted_beg_dixh 52x60 mm" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: 8mm Head" (IFCLABEL)
    Family and Type = "Level: 8mm Head" (IFCLABEL)
    Type = "Level: 8mm Head" (IFCLABEL)
    Type Id = "Level: 8mm Head" (IFCLABEL)
  Other | properties | on 1 type object
    Category = "Lighting Devices" (IFCLABEL)
    Family Name = "RSen_62_LD_FB_movement sensor - 1 channel_beg" (IFCTEXT)
    RSen_E_c01_description = "c01_electrical connector" (IFCTEXT)
    RSen_E_c01_system_type = "Power - Balanced" (IFCTEXT)
    RSen_E_c01_yes_no = TRUE (IFCBOOLEAN)
  Phasing | properties | on 1 object (1 IFCFLOWTERMINAL)
    Phase Created = "New Construction" (IFCLABEL)
  Text | properties | on 1 object (1 IFCFLOWTERMINAL)
    RSen_C_content_manual = "" (IFCTEXT)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Center" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "M_Level Head - Circle: M_Level Head - Circle" (IFCLABEL)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Materials and Finishes | properties | on 1 type object
    RSen_C_material = "RSen_rgb_241_236_225_T00 RAL9010_gen" (IFCLABEL)
  Model Properties | properties | on 1 type object
    Cable Length cm = "-" (IFCTEXT)
    Channel 01 = "lighting control" (IFCTEXT)
    Channel 01 Night light = "-" (IFCTEXT)
    Channel 01 Orientation light = "-" (IFCTEXT)
    Channel 01 Switching power = "2300 W, cos fi = 1, 1150 VA, cos fi = 0.5, 300 W LED, max. inrush current Ip (20 ms) = 165 A, max. inrush current Ip (200 µs) = 800 A" (IFCTEXT)
    Channel 02 = "-" (IFCTEXT)
    Channel 02 Follow up time = "-" (IFCTEXT)
    Channel 02 Orientation light = "-" (IFCTEXT)
    Channel 02 Switch-on threshold lux = "-" (IFCTEXT)
    Channel 02 Switching power = "-" (IFCTEXT)
    Colour = "white mat, similar to RAL9010" (IFCTEXT)
    Data sheet = "https://www.beg-luxomat.com/en/products/luxomat/ceiling-mounted-occupancy-detectors/1-channel/pd11-m-1c-flat/printPage/" (IFCTEXT)
    External power supply Dimensions = "-" (IFCTEXT)
    Housing = "Polycarbonate, UV-resistant" (IFCTEXT)
    KNX Number of PIR sensors = "-" (IFCTEXT)
    KNX Number of light sensors = "-" (IFCTEXT)
    KNX TP 256 = "-" (IFCTEXT)
    Manual = "https://www.beg-luxomat.com/en/products/?jumpurl=uploads/tx_begproducts/jc_medien/web/web_pdf/en-GB/8198_OP_MAN_PD11-M-1C-FLAT-DE_92583_92593_en_V2.pdf&juSecure=1&locationData=236:pages:236&juHash=c916c83f62b39a3fa60750f2ed9cffe4aaa36378" (IFCTEXT)
    Measured Light Output = "-" (IFCTEXT)
    Monitored area of tangential movement on 2,5 m Mounting height m² = "64" (IFCTEXT)
    Mounting height Max m = "5" (IFCTEXT)
    Mounting height Min m = "2" (IFCTEXT)
    Mounting height Recommended m = "2,5" (IFCTEXT)
    Power consumption W = "0,3" (IFCTEXT)
    Power input mA = "-" (IFCTEXT)
    Scenario = "entrance hall, corridor/hallway, staircase, small office, open-plan office/conference room" (IFCTEXT)
    Sensor Depth in mm = "-" (IFCTEXT)
    Sensor Height in mm = "60" (IFCTEXT)
    Sensor Width in mm = "52" (IFCTEXT)
    Settings = "-" (IFCTEXT)
    TBQ_I Ambient_temperature = "-25 °C to +50 °C" (IFCTEXT)
    TBQ_I Detection range = "Detection angle 360°, 9 m on height of 2,5 m" (IFCTEXT)
    TBQ_I Light sensitivity = "20 - 1000 lux" (IFCTEXT)
    TBQ_I Master = TRUE (IFCBOOLEAN)
    TBQ_I Mounting elevation = "0" (IFCTEXT)
    TBQ_I Relay contact channel_01 = "1x µ-contact, NO contact with tungsten pre-make contac" (IFCTEXT)
    TBQ_I Relay contact channel_02 = "" (IFCTEXT)
    TBQ_I Slave = FALSE (IFCBOOLEAN)
    TBQ_I Switch-off delay = "5 min – 30 min, Pulse" (IFCTEXT)
    TBQ_I Type of output = "Switch ON/OFF" (IFCTEXT)
    Temperature Output = "-" (IFCTEXT)