IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "Project Number"
Time stamp: "2021-03-09T11:28:11"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "21.1.21.45 - Exporter 21.1.21.45 - IFC Model Exchange with Archicad 24.0.0.4000"
Application: "Autodesk Revit 2021 (ENU)" version "2021" identifier "Revit" by Organization "Autodesk Revit 2021 (ENU)"

People and organizations
  Person "sebastian.walicki" of Organization (no name given)
  Owner history of Person "sebastian.walicki" of Organization (no name given) | application "Autodesk Revit 2021 (ENU)" version "2021" identifier "Revit" by Organization "Autodesk Revit 2021 (ENU)" | change NOCHANGE | created 1615285691 (2021-03-09T10:28:11Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  MOMENTOFINERTIAUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"
  LINEARFORCEUNIT: derived
  PLANARFORCEUNIT: derived

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 21′ 31.181945″ | longitude -71° 3′ 24.263305″ | elevation above sea level 0.
    IFCBUILDING | postal address: "## Street City, State Zip", "Boston", "MA"
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:8mm Head" | elevation 0.
        contains 1 element
          1 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "RSen_67_LD_FB_movement sensor - 1 channel_beg:93546 - pd4n-bms dali-2 - recessed ceiling mounted, ceiling mounted_beg_dixh 106x72 mm" | object type "RSen_67_LD_FB_movement sensor - 1 channel_beg:93546 - pd4n-bms dali-2 - recessed ceiling mounted, ceiling mounted_beg_dixh 106x72 mm" | names: "RSen_67_LD_FB_movement sensor - 1 channel_beg:93546 - pd4n-bms dali-2 - recessed ceiling mounted, ceiling mounted_beg_dixh 106x72 mm:393253" | material: materials ("RSen_x_rgb 104 104 104 T00 grey_gen", "RSen_rgb_241_236_225_T00 RAL9010_gen", "Glass") | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff, Constraints, Construction

Types
  IFCAIRTERMINALTYPE "RSen_67_LD_FB_movement sensor - 1 channel_beg:93546 - pd4n-bms dali-2 - recessed ceiling mounted, ceiling mounted_beg_dixh 106x72 mm" | 1 occurrence | material: materials ("RSen_x_rgb 000 128 255 T80 blue_gen", "RSen_rgb_241_236_225_T00 RAL9010_gen", "<Unnamed>", "RSen_x_rgb 255 128 128 T80 red_gen", "RSen_rgb_241_236_225_T00 RAL9010_gen", "RSen_x_rgb 104 104 104 T00 grey_gen", "RSen_x_rgb 255 128 128 T80 red_gen", "RSen_x_rgb 000 128 000 T80 green_gen") | property sets: Constraints, Construction, Dimensions, Electrical, Identity Data, Materials and Finishes

Property sets
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "8mm Head" (IFCTEXT)
  Pset_ProductRequirements | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCFLOWTERMINAL) | on 1 type object
    Category = "Lighting Devices" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Level 1" (IFCLABEL)
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Author = "" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCFLOWTERMINAL)
    Mark = "18" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "62.60.10" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Description = "RECESSED CEILING MOUNTED, CEILING MOUNTED" (IFCTEXT)
    Manufacturer = "B.E.G." (IFCTEXT)
    Model = "PD4N-BMS DALI-2" (IFCTEXT)
    OmniClass Number = "" (IFCTEXT)
    OmniClass Title = "" (IFCTEXT)
    RSen_C_code_ETIM = "" (IFCTEXT)
    RSen_C_code_ETIM_URL = "http://prod.etim-international.com/" (IFCTEXT)
    RSen_C_code_article = "93546" (IFCTEXT)
    RSen_C_code_gtin = "4007529935468" (IFCTEXT)
    RSen_C_code_product_class = "PD4N-BMS DALI-2" (IFCTEXT)
    RSen_C_content_creator = "© ThorbiQ" (IFCTEXT)
    RSen_C_content_date_changed = "31/03/2021" (IFCTEXT)
    RSen_C_content_date_issue = "31/03/2021" (IFCTEXT)
    RSen_C_content_provider = "B.E.G." (IFCTEXT)
    RSen_C_content_version = "1.0.0" (IFCTEXT)
    RSen_C_description = "RECESSED CEILING MOUNTED, CEILING MOUNTED" (IFCTEXT)
    RSen_C_model = "PD4N-BMS DALI-2" (IFCTEXT)
    RSen_C_revit_version = "2018" (IFCTEXT)
    RSen_C_type = "PD4N-BMS DALI-2" (IFCTEXT)
    RSen_C_type_comments = "movement sensor" (IFCTEXT)
    TBQ_I BaseKeynote = "62.60.10" (IFCTEXT)
    TBQen_C_IFC_version = "2x3" (IFCTEXT)
    TBQen_C_accessory_01_description = "-" (IFCTEXT)
    TBQen_C_code_product = "93546" (IFCTEXT)
    TBQen_C_data_issue_date = "" (IFCTEXT)
    TBQen_C_license = "Creative Commons Attribution NoDerivs (CC-ND)" (IFCTEXT)
    TBQen_C_license_info = "https://tldrlegal.com/license/creative-commons-attribution-noderivs-(cc-nd)#summary" (IFCTEXT)
    Type Name = "93546 - pd4n-bms dali-2 - recessed ceiling mounted, ceiling mounted_beg_dixh 106x72 mm" (IFCTEXT)
    URL = "https://www.beg-luxomat.com/url.php?fast=93546_en" (IFCTEXT)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
    Client Name = "Owner" (IFCTEXT)
    Project Address = "## Street City, State Zip" (IFCTEXT)
    Project Issue Date = "Issue Date" (IFCTEXT)
    Project Name = "Project Name" (IFCTEXT)
    Project Number = "Project Number" (IFCTEXT)
    Project Status = "Project Status" (IFCTEXT)
  Other | properties | on 1 object (1 IFCFLOWTERMINAL)
    Category = "Lighting Devices" (IFCLABEL)
    Family = "RSen_67_LD_FB_movement sensor - 1 channel_beg: 93546 - pd4n-bms dali-2 - recessed ceiling mounted, ceiling mounted_beg_dixh 106x72 mm" (IFCLABEL)
    Family and Type = "RSen_67_LD_FB_movement sensor - 1 channel_beg: 93546 - pd4n-bms dali-2 - recessed ceiling mounted, ceiling mounted_beg_dixh 106x72 mm" (IFCLABEL)
    Type = "RSen_67_LD_FB_movement sensor - 1 channel_beg: 93546 - pd4n-bms dali-2 - recessed ceiling mounted, ceiling mounted_beg_dixh 106x72 mm" (IFCLABEL)
    Type Id = "RSen_67_LD_FB_movement sensor - 1 channel_beg: 93546 - pd4n-bms dali-2 - recessed ceiling mounted, ceiling mounted_beg_dixh 106x72 mm" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: 8mm Head" (IFCLABEL)
    Family and Type = "Level: 8mm Head" (IFCLABEL)
    Type = "Level: 8mm Head" (IFCLABEL)
    Type Id = "Level: 8mm Head" (IFCLABEL)
  Other | properties | on 1 type object
    Category = "Lighting Devices" (IFCLABEL)
    Family Name = "RSen_67_LD_FB_movement sensor - 1 channel_beg" (IFCTEXT)
    RSen_E_c01_description = "c01_electrical connector" (IFCTEXT)
    TBQen_E_c01_system_type = "Power - Balanced" (IFCTEXT)
    TBQen_E_c01_yes_no = TRUE (IFCBOOLEAN)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Center" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "M_Level Head - Circle: M_Level Head - Circle" (IFCLABEL)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Pset_DistributionFlowElementCommon | properties | on 1 object (1 IFCFLOWTERMINAL) | on 1 type object
    Reference = "RSen_67_LD_FB_movement sensor - 1 channel_beg:93546 - pd4n-bms dali-2 - recessed ceiling mounted, ceiling mounted_beg_dixh 106x72 mm" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCFLOWTERMINAL) | on 1 type object
    Manufacturer = "B.E.G." (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCFLOWTERMINAL) | on 1 type object
    Reference = "RSen_67_LD_FB_movement sensor - 1 channel_beg:93546 - pd4n-bms dali-2 - recessed ceiling mounted, ceiling mounted_beg_dixh 106x72 mm" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCFLOWTERMINAL)
    Elevation from Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "Reference Plane : h_leftright" (IFCTEXT)
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 type object
    Default Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Construction | properties | on 1 object (1 IFCFLOWTERMINAL)
    TBQen_C_GOg = FALSE (IFCBOOLEAN)
    TBQen_C_SOg = TRUE (IFCBOOLEAN)
    TBQen_C_accessory_EE_01 = "none_gen" (IFCLABEL)
    TBQen_C_alignment = "Center" (IFCTEXT)
    TBQen_C_alignment_index = 0 (IFCINTEGER)
    TBQen_C_mounting_height = 2500. (IFCLENGTHMEASURE) [MILLI METRE]
  Construction | properties | on 1 type object
    TBQen_C_SOg_LD_2D = "none" (IFCLABEL)
    TBQen_C_SOg_LD_3D = "standard" (IFCLABEL)
    TBQen_C_accessory_EE_02 = "none_gen" (IFCLABEL)
    TBQen_C_accessory_EE_03 = "none_gen" (IFCLABEL)
    TBQen_C_accessory_EE_04 = "none_gen" (IFCLABEL)
    TBQen_C_accessory_EE_05 = "none_gen" (IFCLABEL)
  Dimensions | properties | on 1 object (1 IFCFLOWTERMINAL)
    Area = 0.481713895549651 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.00956074661211073 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 type object
    RSen_C_diameter = 106. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_C_height = 72. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_C_length = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    RSen_C_width = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Electrical | properties | on 1 object (1 IFCFLOWTERMINAL)
    RSen_E_c01_load_class = "Lighting" (IFCLABEL)
    TBQen_E_c01_power_factor = 1. (IFCREAL)
    TBQen_E_knx_operation_01 = "" (IFCTEXT)
    TBQen_E_knx_operation_02 = "" (IFCTEXT)
    TBQen_E_knx_operation_03 = "" (IFCTEXT)
    TBQen_E_knx_operation_04 = "" (IFCTEXT)
    TBQen_E_knx_operation_05 = "" (IFCTEXT)
    TBQen_E_knx_operation_06 = "" (IFCTEXT)
    TBQen_E_power_factor = 1. (IFCREAL)
  Electrical | properties | on 1 type object
    RSen_E_c01_apparent_power = 0. (IFCPOWERMEASURE) [WATT]
    RSen_E_c01_division_engine = FALSE (IFCBOOLEAN)
    RSen_E_c01_number_of_poles = 1 (IFCINTEGER)
    RSen_E_c01_voltage = 22.5 (IFCELECTRICVOLTAGEMEASURE) [VOLT]
  Electrical - Circuiting | properties | on 1 object (1 IFCFLOWTERMINAL)
    Electrical Data = "c01_electrical connector 23 V/1-0 VA" (IFCTEXT)
  Electrical - Loads | properties | on 1 object (1 IFCFLOWTERMINAL)
    Circuit Number = "" (IFCTEXT)
    Panel = "" (IFCTEXT)
  Graphics | properties | on 1 object (1 IFCFLOWTERMINAL)
    TBQen_C_clearance_zone = FALSE (IFCBOOLEAN)
    TBQen_C_detection_zone_01 = FALSE (IFCBOOLEAN)
    TBQen_C_detection_zone_01_description = "Walking across" (IFCTEXT)
    TBQen_C_detection_zone_02 = FALSE (IFCBOOLEAN)
    TBQen_C_detection_zone_02_description = "Walking towards" (IFCTEXT)
    TBQen_C_detection_zone_03 = FALSE (IFCBOOLEAN)
    TBQen_C_detection_zone_03_description = "Seated activity" (IFCTEXT)
    TBQen_C_logo = FALSE (IFCBOOLEAN)
  Phasing | properties | on 1 object (1 IFCFLOWTERMINAL)
    Phase Created = "New Construction" (IFCLABEL)
  Text | properties | on 1 object (1 IFCFLOWTERMINAL)
    RSen_C_content_manual = "" (IFCTEXT)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Materials and Finishes | properties | on 1 type object
    RSen_C_material = "RSen_rgb_241_236_225_T00 RAL9010_gen" (IFCLABEL)
  Model Properties | properties | on 1 type object
    Cable Length cm = "0" (IFCTEXT)
    Channel 01 = "DALI control" (IFCTEXT)
    Channel 01 Night light = "-" (IFCTEXT)
    Channel 01 Orientation light = "-" (IFCTEXT)
    Channel 01 Switching power = "-" (IFCTEXT)
    Channel 02 = "-" (IFCTEXT)
    Channel 02 Follow up time = "-" (IFCTEXT)
    Channel 02 Orientation light = "-" (IFCTEXT)
    Channel 02 Switch-on threshold lux = "-" (IFCTEXT)
    Channel 02 Switching power = "-" (IFCTEXT)
    Colour = "white mat, similar to RAL9010" (IFCTEXT)
    Data sheet = "-" (IFCTEXT)
    External power supply Dimensions = "-" (IFCTEXT)
    Housing = "Polycarbonate, UV-resistant" (IFCTEXT)
    KNX Number of PIR sensors = "-" (IFCTEXT)
    KNX Number of light sensors = "-" (IFCTEXT)
    KNX TP 256 = "-" (IFCTEXT)
    Manual = "http://beg.luxomat.com/bmeall/93546_man_zz.pdf" (IFCTEXT)
    Measured Light Output = "-" (IFCTEXT)
    Monitored area of tangential movement on 2,5 m Mounting height m² = "450" (IFCTEXT)
    Mounting height Max m = "10" (IFCTEXT)
    Mounting height Min m = "2" (IFCTEXT)
    Mounting height Recommended m = "2,5" (IFCTEXT)
    Power consumption W = "-" (IFCTEXT)
    Power input mA = "7" (IFCTEXT)
    Scenario = "-" (IFCTEXT)
    Sensor Depth in mm = "-" (IFCTEXT)
    Sensor Height in mm = "68" (IFCTEXT)
    Sensor Width in mm = "106" (IFCTEXT)
    Settings = "via DALI-Bus and application which supports DALI multisensors according to IEC62386. parts 101. 103. 303 and 304" (IFCTEXT)
    TBQ_I Ambient_temperature = "-25 °C to +50 °C" (IFCTEXT)
    TBQ_I Detection range = "Detection angle 360°, 24 m on height of 2,5 m" (IFCTEXT)
    TBQ_I Light sensitivity = "10 - 2500 lux" (IFCTEXT)
    TBQ_I Master = TRUE (IFCBOOLEAN)
    TBQ_I Mounting elevation = "0" (IFCTEXT)
    TBQ_I Relay contact channel_01 = "-" (IFCTEXT)
    TBQ_I Relay contact channel_02 = "" (IFCTEXT)
    TBQ_I Slave = FALSE (IFCBOOLEAN)
    TBQ_I Switch-off delay = "-" (IFCTEXT)
    TBQ_I Type of output = "DALI" (IFCTEXT)
    Temperature Output = "-" (IFCTEXT)