IFC building model
Schema: "IFC4"
Description: "IFC4"
File name: "construction"
Time stamp: "2024-07-18T10:22:57"
Application: "WinDoPlan planner" version "1.0" identifier "WinDoPlan" by Organization "VEKA AG"

People and organizations
  Person "WinDoPlan" of Organization "VEKA AG"
  Owner history of Person "WinDoPlan" of Organization "VEKA AG" | application "WinDoPlan planner" version "1.0" identifier "WinDoPlan" by Organization "VEKA AG" | change ADDED | created 1721290977 (2024-07-18T08:22:57Z)

Units
  LENGTHUNIT: MILLI METRE
  PLANEANGLEUNIT: RADIAN

Spatial structure
IFCPROJECT "WinDoPlan" | description "configurator export"
  IFCBUILDING "Default Building" | description "Description of Default Building"
    contains 1 element
      1 x IFCDOOR | type IFCDOORTYPE "VEKAMOTION 82 MAX 3500x2200mm 2-piece door" | names: "VEKAMOTION 82 MAX 3500x2200mm 2-piece door" | descriptions: "VEKA AG VEKAMOTION 82 MAX 3500x2200mm 2-piece door" | property sets: Pset_DoorCommon, Pset_DoorWindowGlazingType, Pset_UserIfcDoor

Types
  IFCDOORTYPE "VEKAMOTION 82 MAX 3500x2200mm 2-piece door" | DOOR | USERDEFINED | 1 occurrence | property sets: panel1, panel2 | description "VEKA AG VEKAMOTION 82 MAX 3500x2200mm 2-piece door"

Property sets
  Pset_DoorCommon | properties | on 1 object (1 IFCDOOR)
    IsExternal = TRUE (IFCBOOLEAN)
    ThermalTransmittance = 0.85243 (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_DoorWindowGlazingType | properties | on 1 object (1 IFCDOOR)
    GlassLayers = 3.00000 (IFCCOUNTMEASURE)
  Pset_UserIfcDoor | properties | on 1 object (1 IFCDOOR)
    Classification = "B4-5-3" (IFCTEXT)
    Manufacturer = "VEKA AG" (IFCTEXT)
    Material = "PVC" (IFCTEXT)
    ProfileSystem = "VEKAMOTION 82 MAX" (IFCTEXT)
    U-value = "0.85243 W/(m²·K)" (IFCTEXT)
    Weight = "355.00000 kg" (IFCTEXT)
  panel1 | predefined | on 1 type object
  panel2 | predefined | on 1 type object