IFC building model
Schema: "IFC4"
Description: "IFC4"
File name: "construction"
Time stamp: "2024-07-18T10:23:21"
Application: "WinDoPlan planner" version "1.0" identifier "WinDoPlan" by Organization "VEKA AG"

People and organizations
  Person "WinDoPlan" of Organization "VEKA AG"
  Owner history of Person "WinDoPlan" of Organization "VEKA AG" | application "WinDoPlan planner" version "1.0" identifier "WinDoPlan" by Organization "VEKA AG" | change ADDED | created 1721291001 (2024-07-18T08:23:21Z)

Units
  LENGTHUNIT: MILLI METRE
  PLANEANGLEUNIT: RADIAN

Spatial structure
IFCPROJECT "WinDoPlan" | description "configurator export"
  IFCBUILDING "Default Building" | description "Description of Default Building"
    contains 1 element
      1 x IFCWINDOW | type IFCWINDOWTYPE "VEKAMOVE 76 2000x2000mm 2-piece window" | names: "VEKAMOVE 76 2000x2000mm 2-piece window" | descriptions: "VEKA AG VEKAMOVE 76 2000x2000mm 2-piece window" | property sets: Pset_WindowCommon, Pset_DoorWindowGlazingType, Pset_UserIfcWindow

Types
  IFCWINDOWTYPE "VEKAMOVE 76 2000x2000mm 2-piece window" | WINDOW | DOUBLE_PANEL_VERTICAL | 1 occurrence | property sets: panel1, panel2 | description "VEKAMOVE 76 2000x2000mm 2-piece window"

Property sets
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    IsExternal = TRUE (IFCBOOLEAN)
    ThermalTransmittance = 0.94424 (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_DoorWindowGlazingType | properties | on 1 object (1 IFCWINDOW)
    GlassLayers = 3.00000 (IFCCOUNTMEASURE)
  Pset_UserIfcWindow | properties | on 1 object (1 IFCWINDOW)
    Classification = "B2-4-1" (IFCTEXT)
    Manufacturer = "VEKA AG" (IFCTEXT)
    Material = "PVC" (IFCTEXT)
    ProfileSystem = "VEKAMOVE 76" (IFCTEXT)
    U-value = "0.94424 W/(m²·K)" (IFCTEXT)
    Weight = "130.00000 kg" (IFCTEXT)
  panel1 | predefined | on 1 type object
  panel2 | predefined | on 1 type object