IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
Time stamp: "2020-04-03T11:44:23"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20160225_1515(x64) - Exporter 17.0.416.0 - Alternate UI 17.12.14.0"
Application: "Autodesk Revit 2017 (ENU)" version "2017" identifier "Revit" by Organization "Autodesk Revit 2017 (ENU)"

People and organizations
  Person "maid.sivac4YEFF" of Organization (no name given)
  Owner history of Person "maid.sivac4YEFF" of Organization (no name given) | application "Autodesk Revit 2017 (ENU)" version "2017" identifier "Revit" by Organization "Autodesk Revit 2017 (ENU)" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | elevation 0.
        contains 2 elements
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basic Wall:Wall 1" | object type "Basic Wall:Wall 1:1557" | names: "Basic Wall:Wall 1:2385" | material: layers "Basic Wall:Wall 1" ("Default Wall" 200.) | property sets: Constraints, Dimensions, Other, Phasing, Structural, Pset_WallCommon
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Operator FD10 - Aluminium" | object type "Operator FD10 - Aluminium" | names: "Door-Closer_Operator-For-Swing-Door_Gilgen-FD10:Operator FD10 - Aluminium:114708" | material: materials ("Metal - Gilgen - Aluminium Satin", "Metal - Gilgen - Stainless Steel Polished", "Plastic - Gilgen - Black") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Constraints, Construction, Data, Dimensions

Types
  IFCWALLTYPE "Basic Wall:Wall 1" | STANDARD | 1 occurrence | material: layers "Basic Wall:Wall 1" ("Default Wall" 200.) | property sets: Analytical Properties, Construction, Graphics, Identity Data, Other
  IFCBUILDINGELEMENTPROXYTYPE "Operator FD10 - Aluminium" | 1 occurrence | material: materials ("Metal - Gilgen - Aluminium Satin", "Metal - Gilgen - Stainless Steel Polished", "Plastic - Gilgen - Black") | property sets: Constraints, General, Identity Data, Materials and Finishes, Other

Property sets
  Constraints | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Base Constraint = "Level: Level 1" (IFCLABEL)
    Base Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Base Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Base is Attached = FALSE (IFCBOOLEAN)
    Location Line = "Wall Centerline" (IFCIDENTIFIER)
    Related to Mass = FALSE (IFCBOOLEAN)
    Room Bounding = TRUE (IFCBOOLEAN)
    Top Extension Distance = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Top is Attached = FALSE (IFCBOOLEAN)
    Unconnected Height = 3000. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "Basic Wall : Wall 1" (IFCTEXT)
    Leaf Opening Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Leaf Opening Angle Restriction = "Up To 105°" (IFCTEXT)
    Leaf Thickness = 50. (IFCLENGTHMEASURE) [MILLI METRE]
    Leaf Thickness Restriction = "Determines Opening Angle Axis Distance" (IFCTEXT)
    Level = "Level: Level 1" (IFCLABEL)
    Lintel Depth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Lintel Depth Restriction = "From 0mm To +250mm" (IFCTEXT)
    Operator Body Offset = 10. (IFCLENGTHMEASURE) [MILLI METRE]
    Operator Body Offset Restriction = "From 10mm To 18mm" (IFCTEXT)
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Constraints | properties | on 1 type object
    Default Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Area = 9. (IFCAREAMEASURE) [SQUARE_METRE]
    Length = 3000. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 1.8 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Area = 0.31407391414468 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.00747163444591287 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    x = 321. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Category = "Walls" (IFCLABEL)
    Family = "Basic Wall: Wall 1" (IFCLABEL)
    Family and Type = "Basic Wall: Wall 1" (IFCLABEL)
    Type = "Basic Wall: Wall 1" (IFCLABEL)
    Type Id = "Basic Wall: Wall 1" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Category = "Generic Models" (IFCLABEL)
    Family = "Door-Closer_Operator-For-Swing-Door_Gilgen-FD10: Operator FD10 - Aluminium" (IFCLABEL)
    Family and Type = "Door-Closer_Operator-For-Swing-Door_Gilgen-FD10: Operator FD10 - Aluminium" (IFCLABEL)
    Schedule Level = "Level: Level 1" (IFCLABEL)
    Type = "Door-Closer_Operator-For-Swing-Door_Gilgen-FD10: Operator FD10 - Aluminium" (IFCLABEL)
    Type Id = "Door-Closer_Operator-For-Swing-Door_Gilgen-FD10: Operator FD10 - Aluminium" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: Level 1" (IFCLABEL)
    Family and Type = "Level: Level 1" (IFCLABEL)
    Type = "Level: Level 1" (IFCLABEL)
    Type Id = "Level: Level 1" (IFCLABEL)
  Other | properties | on 1 type object
    Category = "Walls" (IFCLABEL)
    Family Name = "Basic Wall" (IFCTEXT)
  Other | properties | on 1 type object
    Category = "Generic Models" (IFCLABEL)
    Family Name = "Door-Closer_Operator-For-Swing-Door_Gilgen-FD10" (IFCTEXT)
  Phasing | properties | on 2 objects (1 IFCBUILDINGELEMENTPROXY, 1 IFCWALLSTANDARDCASE)
    Phase Created = "New Construction" (IFCLABEL)
  Structural | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    Enable Analytical Model = FALSE (IFCBOOLEAN)
    Structural = FALSE (IFCBOOLEAN)
    Structural Usage = "Non-bearing" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Wall 1" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "Operator FD10 - Aluminium" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    ArticleNumber = "Standard" (IFCIDENTIFIER)
    Manufacturer = "Gilgen" (IFCLABEL)
  Construction | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Operator Axle Extension I = "+0 (mm)" (IFCLABEL)
    Operator Body Placement I = "On Frame" (IFCLABEL)
    Operator Rod Types I = "Standard Rod" (IFCLABEL)
  Construction | properties | on 1 type object
    Function = "Exterior" (IFCIDENTIFIER)
    Width = 200. (IFCLENGTHMEASURE) [MILLI METRE]
    Wrapping at Ends = "None" (IFCIDENTIFIER)
    Wrapping at Inserts = "Do not wrap" (IFCIDENTIFIER)
  Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Article Number = "Standard" (IFCTEXT)
    Operator Assembly = "Operator with Standard Rod, placed on door frame or wall above the door frame" (IFCTEXT)
    Operator Function = "Push" (IFCTEXT)
    Rod Type = "Standard Rod" (IFCTEXT)
  Visibility | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Alignment Symbol = TRUE (IFCBOOLEAN)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Type Name = "Wall 1" (IFCTEXT)
  Identity Data | properties | on 1 type object
    Assembly Code = "E10" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Description = "" (IFCTEXT)
    Keynote = "08700" (IFCTEXT)
    Manufacturer = "Gilgen" (IFCTEXT)
    Model = "Door Operator FD10" (IFCTEXT)
    OmniClass Number = "" (IFCTEXT)
    OmniClass Title = "" (IFCTEXT)
    Product Guid = "ad6d4fb3-5188-4a42-9f31-05ed5f2be77f" (IFCTEXT)
    Product data url = "https://bimobject.com/gilgen/product/FD_10" (IFCTEXT)
    Type Comments = "Gilgen Door Operator FD10, with aluminium covering" (IFCTEXT)
    Type Name = "Operator FD10 - Aluminium" (IFCTEXT)
    URL = "https://www.gilgendoorsystems.com/en" (IFCTEXT)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
  Graphics | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Graphics | properties | on 1 type object
    Coarse Scale Fill Color = 0 (IFCINTEGER)
  Analytical Properties | properties | on 1 type object
    Absorptance = 0.1 (IFCREAL)
    Roughness = 1 (IFCINTEGER)
  General | properties | on 1 type object
    Edition number = 1 (IFCINTEGER)
  Materials and Finishes | properties | on 1 type object
    Product Material = "Metal - Gilgen - Aluminium Satin" (IFCLABEL)