IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
File name: "Project Number"
Time stamp: "2019-02-07T14:37:56"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20160512_1515(x64) - Exporter 2015.0.2016.0512 - Default UI"
Application: "Autodesk Revit 2015 (ENU)" version "2015" identifier "Revit" by Organization "Autodesk Revit 2015 (ENU)"

People and organizations
  Person "Irnes.Duran" of Organization (no name given)
  Owner history of Person "Irnes.Duran" of Organization (no name given) | application "Autodesk Revit 2015 (ENU)" version "2015" identifier "Revit" by Organization "Autodesk Revit 2015 (ENU)" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  PRESSUREUNIT: PASCAL

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 51° 30′ 0.549316″ | longitude -0° 7′ 34.450321″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "Westminster", "London", "UK"
      IFCBUILDINGSTOREY "Level 0" | long name "Level 0" | elevation 0.
        contains 5 elements
          5 x IFCFLOWTERMINAL | object type "CeraWall Individual 1000mm" | names: "Plumbing_Drainage_Dallmer_CeraWall-Individual:CeraWall Individual 1000mm:291756", "Plumbing_Drainage_Dallmer_CeraWall-Individual:CeraWall Individual 1000mm:291854", "Plumbing_Drainage_Dallmer_CeraWall-Individual:CeraWall Individual 1000mm:291875" (+2 more) | material: materials ("PVC - Dallmer - Piping", "Steel - Dallmer - DallFlex - Black", "Plastic - Dallmer - DallFlex - Black", "Plastic - Dallmer - DallFlex - Blue", "Plastic - Dallmer - DallFlex - Gray", "Stainless Steel - Dallmer - DallFlex - Satin"); materials ("PVC - Dallmer - Piping", "Plastic - Dallmer - DallFlex - White", "Plastic - Dallmer - DallFlex - Black", "Plastic - Dallmer - DallFlex - Blue", "Plastic - Dallmer - DallFlex - Gray", "Stainless Steel - Dallmer - DallFlex - Satin"); materials ("PVC - Dallmer - Piping", "Plastic - Dallmer - DallFlex - Black", "Steel - Dallmer - DallFlex - Black", "Plastic - Dallmer - DallFlex - Gray", "Plastic - Dallmer - DallFlex - Blue", "Stainless Steel - Dallmer - DallFlex - Satin") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Constraints, Construction, Dimensions, Graphics

Property sets
  Other | properties | on 5 objects (5 IFCFLOWTERMINAL)
    Category = "Plumbing Fixtures" (IFCLABEL)
    Family = "Plumbing_Drainage_Dallmer_CeraWall-Individual: CeraWall Individual 1000mm" (IFCLABEL)
    Family and Type = "Plumbing_Drainage_Dallmer_CeraWall-Individual: CeraWall Individual 1000mm" (IFCLABEL)
    Host Id = "Floor: Floor-Grnd-Susp_65Scr-80Ins-100Blk-75PC" (IFCLABEL)
    Type = "Plumbing_Drainage_Dallmer_CeraWall-Individual: CeraWall Individual 1000mm" (IFCLABEL)
    Type Id = "Plumbing_Drainage_Dallmer_CeraWall-Individual: CeraWall Individual 1000mm" (IFCLABEL)
    t1 = 4.5 (IFCLENGTHMEASURE) [MILLI METRE]
    t2 = 4. (IFCLENGTHMEASURE) [MILLI METRE]
    v_h = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Other | properties | on 5 objects (5 IFCFLOWTERMINAL)
    Category = "Plumbing Fixtures" (IFCLABEL)
    Family Name = "Plumbing_Drainage_Dallmer_CeraWall-Individual" (IFCTEXT)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
    Client Name = "Owner" (IFCTEXT)
    Project Address = "Enter address here" (IFCTEXT)
    Project Issue Date = "Issue Date" (IFCTEXT)
    Project Name = "Project Name" (IFCTEXT)
    Project Number = "Project Number" (IFCTEXT)
    Project Status = "Project Status" (IFCTEXT)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: Circle Head - Project Datum" (IFCLABEL)
    Family and Type = "Level: Circle Head - Project Datum" (IFCLABEL)
    Type = "Level: Circle Head - Project Datum" (IFCLABEL)
    Type Id = "Level: Circle Head - Project Datum" (IFCLABEL)
  Identity Data | properties | on 5 objects (5 IFCFLOWTERMINAL)
    Assembly Code = "D2030300" (IFCTEXT)
    Assembly Description = "Floor Drains" (IFCTEXT)
    Description = "Shower Channel" (IFCTEXT)
    EAN code = "" (IFCTEXT)
    Installation instructions = "http://www.dallmer.de/wAssets/docs/de/montageanleitungen/Montageanleitung-348535214.pdf" (IFCTEXT)
    Keynote = "15150.A2" (IFCTEXT)
    Manufacturer = "Dallmer" (IFCTEXT)
    Model = "CeraWall Individual" (IFCTEXT)
    OmniClass Number = "23.45.55.21" (IFCTEXT)
    OmniClass Title = "Drains (Wastes)" (IFCTEXT)
    Product Guid = "b38b1987-e3fb-46f7-b352-08eadb134640" (IFCTEXT)
    Product certification = "" (IFCTEXT)
    Product data url = "https://bimobject.com/dallmer/product/shower-channels-cerawall-individual-535269535665" (IFCTEXT)
    Product url = "http://www.dallmer.de/wAssets/docs/de/pdb/dallmer_acc_535269.pdf" (IFCTEXT)
    Technical description = "" (IFCTEXT)
    Type Name = "CeraWall Individual 1000mm" (IFCTEXT)
    URL = "http://www.dallmer.com/en/" (IFCTEXT)
    Youtube clip = "https://www.youtube.com/embed/Qr2IHvfAQqs?rel=0&autoplay=1&viewmode=blank" (IFCTEXT)
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Author = "" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Circle Head - Project Datum" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCFLOWTERMINAL)
    Mark = "1" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCFLOWTERMINAL)
    Mark = "2" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCFLOWTERMINAL)
    Mark = "3" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCFLOWTERMINAL)
    Mark = "4" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCFLOWTERMINAL)
    Mark = "5" (IFCTEXT)
  Identity Data: 1 more content on 1 objects not shown
  Pset_ManufacturerTypeInformation | properties | on 5 objects (5 IFCFLOWTERMINAL)
    Manufacturer = "Dallmer" (IFCLABEL)
  Pset_DistributionFlowElementCommon | properties | on 5 objects (5 IFCFLOWTERMINAL)
    Reference = "CeraWall Individual 1000mm" (IFCIDENTIFIER)
  Constraints | properties | on 3 objects (3 IFCFLOWTERMINAL)
    Leg Warning Visiblity = FALSE (IFCBOOLEAN)
    Length Warning Visiblity = FALSE (IFCBOOLEAN)
    Level = "Level: Level 0" (IFCLABEL)
  Constraints | properties | on 2 objects (2 IFCFLOWTERMINAL)
    Leg Warning Visiblity = TRUE (IFCBOOLEAN)
    Length Warning Visiblity = FALSE (IFCBOOLEAN)
    Level = "Level: Level 0" (IFCLABEL)
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Construction | properties | on 1 object (1 IFCFLOWTERMINAL)
    Article Number Cover Plate = "535023" (IFCTEXT)
    Article Number Drain Body = "539007" (IFCTEXT)
    Article Number Fire Protection = "Not available for selected drain body type" (IFCTEXT)
    Article Number Shower Channel = "535214" (IFCTEXT)
    Article Number Shower Underlay = "" (IFCTEXT)
    Article Number Sound Insulation = "" (IFCTEXT)
    Cover Plate Usage = "For flooring with unfinished cut edges (e.g. glazed tiles)" (IFCTEXT)
    Drain Body Type = "DN 50" (IFCLABEL)
    Fire Protection System = FALSE (IFCBOOLEAN)
    Outlet Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Outlet Position = "Concentric" (IFCLABEL)
    Shower Channel Finish = "satin stainless steel 535023" (IFCLABEL)
    Shower Underlay = FALSE (IFCBOOLEAN)
    Shower Underlay Type = "1000 x 1000 mm, DN 50" (IFCLABEL)
    Sound Insulation = FALSE (IFCBOOLEAN)
  Construction | properties | on 1 object (1 IFCFLOWTERMINAL)
    Article Number Cover Plate = "535023" (IFCTEXT)
    Article Number Drain Body = "539014" (IFCTEXT)
    Article Number Fire Protection = "Not available for selected drain body type" (IFCTEXT)
    Article Number Shower Channel = "535214" (IFCTEXT)
    Article Number Shower Underlay = "" (IFCTEXT)
    Article Number Sound Insulation = "" (IFCTEXT)
    Cover Plate Usage = "For flooring with unfinished cut edges (e.g. glazed tiles)" (IFCTEXT)
    Drain Body Type = "Plan DN 40" (IFCLABEL)
    Fire Protection System = FALSE (IFCBOOLEAN)
    Outlet Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Outlet Position = "Concentric" (IFCLABEL)
    Shower Channel Finish = "satin stainless steel 535023" (IFCLABEL)
    Shower Underlay = FALSE (IFCBOOLEAN)
    Shower Underlay Type = "1000 x 1000 mm, DN 50" (IFCLABEL)
    Sound Insulation = FALSE (IFCBOOLEAN)
  Construction | properties | on 1 object (1 IFCFLOWTERMINAL)
    Article Number Cover Plate = "535023" (IFCTEXT)
    Article Number Drain Body = "539304" (IFCTEXT)
    Article Number Fire Protection = "Not available for selected drain body type" (IFCTEXT)
    Article Number Shower Channel = "535214" (IFCTEXT)
    Article Number Shower Underlay = "" (IFCTEXT)
    Article Number Sound Insulation = "Sound insulation not available for selected drain body type" (IFCTEXT)
    Cover Plate Usage = "For flooring with unfinished cut edges (e.g. glazed tiles)" (IFCTEXT)
    Drain Body Type = "EPS Assembled DN 50" (IFCLABEL)
    Fire Protection System = FALSE (IFCBOOLEAN)
    Outlet Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Outlet Position = "Concentric" (IFCLABEL)
    Shower Channel Finish = "satin stainless steel 535023" (IFCLABEL)
    Shower Underlay = FALSE (IFCBOOLEAN)
    Shower Underlay Type = "1000 x 1000 mm, DN 50" (IFCLABEL)
    Sound Insulation = FALSE (IFCBOOLEAN)
  Construction | properties | on 1 object (1 IFCFLOWTERMINAL)
    Article Number Cover Plate = "535023" (IFCTEXT)
    Article Number Drain Body = "539311" (IFCTEXT)
    Article Number Fire Protection = "Not available for selected drain body type" (IFCTEXT)
    Article Number Shower Channel = "535214" (IFCTEXT)
    Article Number Shower Underlay = "" (IFCTEXT)
    Article Number Sound Insulation = "Sound insulation not available for selected drain body type" (IFCTEXT)
    Cover Plate Usage = "For flooring with unfinished cut edges (e.g. glazed tiles)" (IFCTEXT)
    Drain Body Type = "Plan EPS Assembled DN 40" (IFCLABEL)
    Fire Protection System = FALSE (IFCBOOLEAN)
    Outlet Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Outlet Position = "Concentric" (IFCLABEL)
    Shower Channel Finish = "satin stainless steel 535023" (IFCLABEL)
    Shower Underlay = FALSE (IFCBOOLEAN)
    Shower Underlay Type = "1000 x 1000 mm, DN 50" (IFCLABEL)
    Sound Insulation = FALSE (IFCBOOLEAN)
  Construction | properties | on 1 object (1 IFCFLOWTERMINAL)
    Article Number Cover Plate = "535023" (IFCTEXT)
    Article Number Drain Body = "539076" (IFCTEXT)
    Article Number Fire Protection = "" (IFCTEXT)
    Article Number Shower Channel = "535214" (IFCTEXT)
    Article Number Shower Underlay = "" (IFCTEXT)
    Article Number Sound Insulation = "Sound insulation not available for selected drain body type" (IFCTEXT)
    Cover Plate Usage = "For flooring with unfinished cut edges (e.g. glazed tiles)" (IFCTEXT)
    Drain Body Type = "Vertical DN 50" (IFCLABEL)
    Fire Protection System = FALSE (IFCBOOLEAN)
    Outlet Angle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Outlet Position = "Concentric" (IFCLABEL)
    Shower Channel Finish = "satin stainless steel 535023" (IFCLABEL)
    Shower Underlay = FALSE (IFCBOOLEAN)
    Shower Underlay Type = "1000 x 1000 mm, DN 50" (IFCLABEL)
    Sound Insulation = FALSE (IFCBOOLEAN)
  Dimensions | properties | on 5 objects (5 IFCFLOWTERMINAL)
    Length = 1000. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCFLOWTERMINAL)
    Area = 2.834684108764 (IFCAREAMEASURE) [SQUARE_METRE]
    Drain Body Height = 90. (IFCLENGTHMEASURE) [MILLI METRE]
    Floor Finish Thickness = 15. (IFCLENGTHMEASURE) [MILLI METRE]
    Leg Height = 90. (IFCLENGTHMEASURE) [MILLI METRE]
    Leg Height Available = "90<Leg Height<143" (IFCTEXT)
    Pipe Diameter = 50. (IFCLENGTHMEASURE) [MILLI METRE]
    Suitable for Floor Finish = "12-24mm" (IFCTEXT)
    Volume = 0.105624893982265 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCFLOWTERMINAL)
    Area = 2.93916090649734 (IFCAREAMEASURE) [SQUARE_METRE]
    Drain Body Height = 65. (IFCLENGTHMEASURE) [MILLI METRE]
    Floor Finish Thickness = 15. (IFCLENGTHMEASURE) [MILLI METRE]
    Leg Height = 90. (IFCLENGTHMEASURE) [MILLI METRE]
    Leg Height Available = "65<Leg Height<143" (IFCTEXT)
    Pipe Diameter = 40. (IFCLENGTHMEASURE) [MILLI METRE]
    Suitable for Floor Finish = "12-24mm" (IFCTEXT)
    Volume = 0.108395966836082 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCFLOWTERMINAL)
    Area = 2.834684108764 (IFCAREAMEASURE) [SQUARE_METRE]
    Drain Body Height = 90. (IFCLENGTHMEASURE) [MILLI METRE]
    Floor Finish Thickness = 15. (IFCLENGTHMEASURE) [MILLI METRE]
    Leg Height = 90. (IFCLENGTHMEASURE) [MILLI METRE]
    Leg Height Available = "Leg Height=0" (IFCTEXT)
    Pipe Diameter = 50. (IFCLENGTHMEASURE) [MILLI METRE]
    Suitable for Floor Finish = "12-24mm" (IFCTEXT)
    Volume = 0.105624893982265 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCFLOWTERMINAL)
    Area = 2.93916090649734 (IFCAREAMEASURE) [SQUARE_METRE]
    Drain Body Height = 65. (IFCLENGTHMEASURE) [MILLI METRE]
    Floor Finish Thickness = 15. (IFCLENGTHMEASURE) [MILLI METRE]
    Leg Height = 90. (IFCLENGTHMEASURE) [MILLI METRE]
    Leg Height Available = "Leg Height=0" (IFCTEXT)
    Pipe Diameter = 40. (IFCLENGTHMEASURE) [MILLI METRE]
    Suitable for Floor Finish = "12-24mm" (IFCTEXT)
    Volume = 0.108395966836082 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCFLOWTERMINAL)
    Area = 2.8085000943106 (IFCAREAMEASURE) [SQUARE_METRE]
    Drain Body Height = 30. (IFCLENGTHMEASURE) [MILLI METRE]
    Floor Finish Thickness = 15. (IFCLENGTHMEASURE) [MILLI METRE]
    Leg Height = 90. (IFCLENGTHMEASURE) [MILLI METRE]
    Leg Height Available = "30<Leg Height<143" (IFCTEXT)
    Pipe Diameter = 50. (IFCLENGTHMEASURE) [MILLI METRE]
    Suitable for Floor Finish = "12-24mm" (IFCTEXT)
    Volume = 0.105578282959995 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Graphics | properties | on 5 objects (5 IFCFLOWTERMINAL)
    Symbolic Representation = TRUE (IFCBOOLEAN)
  Graphics | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Centre" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "Anno_Level_Head_Circle: Standard" (IFCLABEL)
    Symbol at End 1 Default = TRUE (IFCBOOLEAN)
    Symbol at End 2 Default = FALSE (IFCBOOLEAN)
  Mechanical | properties | on 2 objects (2 IFCFLOWTERMINAL)
    Flow Rate = 0.0008 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    System Abbreviation = "" (IFCTEXT)
    System Classification = "Sanitary" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Mechanical | properties | on 2 objects (2 IFCFLOWTERMINAL)
    Flow Rate = 0.0005 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    System Abbreviation = "" (IFCTEXT)
    System Classification = "Sanitary" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Mechanical | properties | on 1 object (1 IFCFLOWTERMINAL)
    Flow Rate = 0.001 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    System Abbreviation = "" (IFCTEXT)
    System Classification = "Sanitary" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Phasing | properties | on 5 objects (5 IFCFLOWTERMINAL)
    Phase Created = "New Construction" (IFCLABEL)
  Materials and Finishes | properties | on 5 objects (5 IFCFLOWTERMINAL)
    Material main = "Stainless steel" (IFCTEXT)
    Material secondary = "Polypropylene" (IFCTEXT)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
  General | properties | on 5 objects (5 IFCFLOWTERMINAL)
    Brand url = "http://www.dallmer.com/en/" (IFCTEXT)
    Date of publishing = "" (IFCTEXT)
    Design country = "Germany" (IFCTEXT)
    Edition number = 1 (IFCINTEGER)
    Manufacturer country = "Germany" (IFCTEXT)
    Manufacturer name = "Dallmer" (IFCTEXT)
    Nominal height = 0. (IFCREAL)
    Nominal width = 0. (IFCREAL)
    Product SKU = "shower-channels-cerawall-individual-535269535665" (IFCTEXT)
    Product family = "Shower channel" (IFCTEXT)
    Product group = "DallFlex" (IFCTEXT)
    QR code = "http://bimobject.com/dallmer/product/shower-channels-cerawall-individual-535269535665" (IFCTEXT)
    Region Africa = "AO, BF, BI, BJ, BW, CD, CF, CG, CI, CM, CV, DJ, DZ, EH, ER, ET, GA, GH, GM, GN, GQ, GW, KE, KM, LR, LS, LY, MA, MG, ML, MR, MU, MW, MZ, NA, NE, NG, RE, RW, SC, SD, SH, SL, SN, SO, SS, ST, SZ, TD, TG, TN, TZ, UG, YT, ZA, ZM, ZW" (IFCTEXT)
    Region Antarctica = "BV, GS, HM, TF" (IFCTEXT)
    Region Asia = "AM, AZ, BD, BN, BT, CC, CN, CX, GE, HK, ID, IN, IO, JP, KG, KH, KP, KR, KZ, LA, LK, MM, MN, MO, MV, MY, NP, PH, PK, SG, TH, TJ, TM, TW, UZ, VN" (IFCTEXT)
    Region Europe = "AD, AL, AT, AX, BA, BE, BG, BY, CH, CY, CZ, DE, DK, EE, ES, FI, FO, FR, GB, GG, GI, GR, HR, HU, IE, IM, IS, IT, JE, LI, LT, LU, LV, MC, MD, ME, MK, MT, NL, NO, PL, PT, RO, RS, RU, SE, SI, SJ, SK, SM, UA, VA" (IFCTEXT)
    Region Middle East = "AE, AF, BH, EG, IL, IQ, IR, JO, KW, LB, OM, PS, QA, SA, SY, TR, YE" (IFCTEXT)
    Region North America = "AG, AI, AW, BB, BL, BM, BQ, BS, BZ, CA, CR, CU, CW, DM, DO, GD, GL, GP, GT, HN, HT, JM, KN, KY, LC, MF, MQ, MS, MX, NI, PA, PM, PR, SV, SX, TC, TT, US, VC, VG, VI" (IFCTEXT)
    Region Oceania = "AS, AU, CK, FJ, FM, GU, KI, MH, MP, NC, NF, NR, NU, NZ, PF, PG, PN, PW, SB, TK, TL, TO, TV, UM, WF, WS, VU" (IFCTEXT)
    Region South America = "AR, BO, BR, CL, CO, EC, FK, GF, GY, PE, PY, SR, UY, VE" (IFCTEXT)
    Weight Net (Kg) = 0. (IFCREAL)