IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "Project Number"
Time stamp: "2021-12-01T14:24:42"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20210416_1515(x64) - Exporter 19.2.30.41 - Alternate UI 19.2.30.41"
Application: "Autodesk Revit 2019 (ENG)" version "2019" identifier "Revit" by Organization "Autodesk Revit 2019 (ENG)"

People and organizations
  Person "Josh.BateyDYJ6D" of Organization (no name given)
  Owner history of Person "Josh.BateyDYJ6D" of Organization (no name given) | application "Autodesk Revit 2019 (ENG)" version "2019" identifier "Revit" by Organization "Autodesk Revit 2019 (ENG)" | change NOCHANGE | created 1638368682 (2021-12-01T14:24:42Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 51° 30′ 23.112487″ | longitude -0° 7′ 37.956022″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "London", "London", "United Kingdom"
      IFCBUILDINGSTOREY "Level 0" | long name "Level 0" | elevation 0.
        contains 1 element
          1 x IFCFLOWTERMINAL | type IFCSANITARYTERMINALTYPE "Fundo Riolito neo 1200x1000x50mm_900mmChannel" | object type "Fundo Riolito neo 1200x1000x50mm_900mmChannel" | names: "NBS_wediSystems-UK-Ltd_ShwrTrys_wediFundoRiolitoneofloorelement:Fundo Riolito neo 1200x1000x50mm_900mmChannel:317745" | material: "NBS_wedi_PolystyreneExpanded" | property sets: COBie

Types
  IFCSANITARYTERMINALTYPE "Fundo Riolito neo 1200x1000x50mm_900mmChannel" | SHOWER | 1 occurrence | material: "NBS_wedi_PolystyreneExpanded" | property sets: BOS_General, NBS_Data, Pset_SanitaryTerminalTypeShower, IFC, COBie

Property sets
  COBie | properties | on 1 object (1 IFCFLOWTERMINAL)
    AssetIdentifier = "n/a" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "Suitable for wheelchair users" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Pr_40_20_06_84:Shower trays" (IFCTEXT)
    CodePerformance = "EN 1606, EN 826, EN 13164, EN 13501" (IFCTEXT)
    Color = "n/a" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Neo floor-level shower element with a channel drain" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "30" (IFCTEXT)
    Features = "Fully watertight, close to wall drainage,extremely flat surface, suitable for wheelchair users" (IFCTEXT)
    Finish = "n/a" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Manufacturer = "technical@wedi.co.uk" (IFCTEXT)
    Material = "A waterproof extruded polystyrene rigid foam core with a special, resistant and glass fibre reinforced cement coating" (IFCTEXT)
    ModelNumber = "075100008" (IFCTEXT)
    ModelReference = "wedi Fundo Riolito neo floor element" (IFCTEXT)
    Name = "ShowerTrays_wediFundoRiolitoneofloorelement_1200x1000x50mm_900mmChannel_wediSystemsLtd" (IFCTEXT)
    NominalHeight = 50.000000076 (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 1200. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 1000. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "Square" (IFCTEXT)
    Size = "1200 x 1000 x 50 mm" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "n/a" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  BOS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_wediSystemsLtd_ShowerTrays_wediFundoRiolitoneofloorelement_1200x1000x50mm_900mmChannel" (IFCTEXT)
    ManufacturerName = "wedi Systems (UK) Ltd" (IFCTEXT)
    ManufacturerURL = "https://www.wedi.de/uk/" (IFCTEXT)
    NBSCertification = "www.nationalbimlibrary.com/cert/i1a4lmf2" (IFCTEXT)
    NBSDescription = "Shower trays" (IFCTEXT)
    NBSReference = "45-35-70/336" (IFCTEXT)
    ProductInformation = "https://www.wedi.de/en/products/building-systems/floor-level-showers/fundo-riolito-neo" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2015Code = "Pr_40_20_06_84" (IFCTEXT)
    Uniclass2015Title = "Shower trays" (IFCTEXT)
    Uniclass2015Version = "Products v1.16" (IFCTEXT)
    Version = "3" (IFCTEXT)
  NBS_Data | properties | on 1 type object
    Applications = "Private housing, publicly accessible buildings and workplaces" (IFCTEXT)
    GlassMosaicSize = "20 x 20 mm" (IFCTEXT)
    GrossDensity = "n/a" (IFCTEXT)
    TemperatureLimit = "n/a" (IFCTEXT)
    ThermalConductivity = "n/a" (IFCTEXT)
    TileSize = "50 x 50 mm" (IFCTEXT)
    WasteHole = "DN50" (IFCTEXT)
  Pset_SanitaryTerminalTypeShower | properties | on 1 type object
    DrainSize = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    ShowerHeadDescription = "n/a" (IFCTEXT)
    ShowerType = "n/a" (IFCTEXT)
  IFC | properties | on 1 type object
    IfcExportAs = "IfcSanitaryTerminalType" (IFCTEXT)
    IfcExportType = "SHOWER" (IFCTEXT)