IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "2018_01"
Time stamp: "2022-03-11T15:34:54"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20190327_2315(x64) - Exporter 20.0.0.377 - Alternativ-UI 20.0.0.377"
Application: "Autodesk Revit 2020 (DEU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (DEU)"

People and organizations
  Person "christina.baartQ88XW" of Organization (no name given)
  Owner history of Person "christina.baartQ88XW" of Organization (no name given) | application "Autodesk Revit 2020 (DEU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (DEU)" | change NOCHANGE | created 1647009291 (2022-03-11T14:34:51Z)

Units
  LENGTHUNIT: METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "2018_01" | phase "Projekt Status"
  IFCSITE "Default" | latitude 48° 8′ 15.359802″ | longitude 11° 34′ 47.783432″ | elevation above sea level 0.
    IFCBUILDING
      contains 27 elements
        2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basiswand:Ziegel+WD hart 300+160" | object type "Basiswand:Ziegel+WD hart 300+160" | names: "Basiswand:Ziegel+WD hart 300+160:2449583", "Basiswand:Ziegel+WD hart 300+160:2454283" | material: layers "Basiswand:Ziegel+WD hart 300+160" ("Dämmung - hart" 0.16, "Mauerwerk - Ziegel" 0.3) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
        12 x IFCOPENINGELEMENT | object type "Opening" | names: "Basiswand:Ziegel+WD hart 300+160:2449583", "Basiswand:Ziegel 200:2453988", "Basiswand:Ziegel+WD hart 300+160:2454283" | property sets: Pset_QuantityTakeOff, Pset_OpeningElementCommon
        1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "ASN-1" | object type "SystemSchroeders_Wandklappe:ASN-1" | names: "SystemSchroeders_Wandklappe:ASN-1:2453670" | material: "Edelstahl" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
        1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "EIS-11" | object type "SystemSchroeders_Wandklappe:EIS-11" | names: "SystemSchroeders_Wandklappe:EIS-11:2453757" | material: "Edelstahl" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
        1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "ESN-1" | object type "SystemSchroeders_Wandklappe:ESN-1" | names: "SystemSchroeders_Wandklappe:ESN-1:2453800" | material: "Edelstahl" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
        1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "ISN-1" | object type "SystemSchroeders_Wandklappe:ISN-1" | names: "SystemSchroeders_Wandklappe:ISN-1:2453853" | material: "Edelstahl" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
        1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "Basiswand:Ziegel 200" | object type "Basiswand:Ziegel 200" | names: "Basiswand:Ziegel 200:2453988" | material: layers "Basiswand:Ziegel 200" ("Mauerwerk - Ziegel" 0.2) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
        1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "RSN-1" | object type "SystemSchroeders_Wandklappe:RSN-1" | names: "SystemSchroeders_Wandklappe:RSN-1:2454036" | material: "Edelstahl" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
        1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "RSN-1 CE" | object type "SystemSchroeders_Wandklappe:RSN-1 CE" | names: "SystemSchroeders_Wandklappe:RSN-1 CE:2454102" | material: "Edelstahl" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
        1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "SN-1" | object type "SystemSchroeders_Wandklappe:SN-1" | names: "SystemSchroeders_Wandklappe:SN-1:2454167" | material: "Edelstahl" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
        1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "TSN-1" | object type "SystemSchroeders_Wandklappe:TSN-1" | names: "SystemSchroeders_Wandklappe:TSN-1:2454198" | material: "Edelstahl" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
        1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "TSN-1 CE" | object type "SystemSchroeders_Wandklappe:TSN-1 CE" | names: "SystemSchroeders_Wandklappe:TSN-1 CE:2454302" | material: "Edelstahl" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
        1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "TSN-3 CE" | object type "SystemSchroeders_Wandklappe:TSN-3 CE" | names: "SystemSchroeders_Wandklappe:TSN-3 CE:2454363" | material: "Edelstahl" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
        1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "TSN-11" | object type "SystemSchroeders_Wandklappe:TSN-11" | names: "SystemSchroeders_Wandklappe:TSN-11:2454416" | material: "Edelstahl" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
        1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "TSN-11 CE" | object type "SystemSchroeders_Wandklappe:TSN-11 CE" | names: "SystemSchroeders_Wandklappe:TSN-11 CE:2454455" | material: "Edelstahl" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff

Types
  IFCWALLTYPE "Basiswand:Ziegel+WD hart 300+160" | STANDARD | 2 occurrences | material: layers "Basiswand:Ziegel+WD hart 300+160" ("Dämmung - hart" 0.16, "Mauerwerk - Ziegel" 0.3) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "ASN-1" | 1 occurrence | material: "Edelstahl" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "EIS-11" | 1 occurrence | material: "Edelstahl" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "ESN-1" | 1 occurrence | material: "Edelstahl" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "ISN-1" | 1 occurrence | material: "Edelstahl" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
  IFCWALLTYPE "Basiswand:Ziegel 200" | STANDARD | 1 occurrence | material: layers "Basiswand:Ziegel 200" ("Mauerwerk - Ziegel" 0.2) | property sets: Pset_QuantityTakeOff, Pset_ReinforcementBarPitchOfWall, Pset_WallCommon
  IFCBUILDINGELEMENTPROXYTYPE "RSN-1" | 1 occurrence | material: "Edelstahl" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "RSN-1 CE" | 1 occurrence | material: "Edelstahl" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "SN-1" | 1 occurrence | material: "Edelstahl" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "TSN-1" | 1 occurrence | material: "Edelstahl" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "TSN-1 CE" | 1 occurrence | material: "Edelstahl" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "TSN-3 CE" | 1 occurrence | material: "Edelstahl" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "TSN-11" | 1 occurrence | material: "Edelstahl" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff
  IFCBUILDINGELEMENTPROXYTYPE "TSN-11 CE" | 1 occurrence | material: "Edelstahl" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff

Property sets
  Pset_QuantityTakeOff | properties | on 10 objects (8 IFCOPENINGELEMENT, 2 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "Ziegel+WD hart 300+160" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 5 objects (4 IFCOPENINGELEMENT, 1 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "Ziegel 200" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "ASN-1" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "EIS-11" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "ESN-1" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "ISN-1" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "RSN-1" (IFCIDENTIFIER)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "RSN-1 CE" (IFCIDENTIFIER)
  Pset_QuantityTakeOff: 6 more contents on 6 objects not shown
  Pset_ReinforcementBarPitchOfWall | properties | on 2 objects (2 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "Ziegel+WD hart 300+160" (IFCLABEL)
  Pset_ReinforcementBarPitchOfWall | properties | on 1 object (1 IFCWALLSTANDARDCASE) | on 1 type object
    Reference = "Ziegel 200" (IFCLABEL)
  Pset_WallCommon | properties | on 2 objects (2 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Ziegel+WD hart 300+160" (IFCIDENTIFIER)
    ThermalTransmittance = 0.154285714285714 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 1 object (1 IFCWALLSTANDARDCASE)
    ExtendToStructure = FALSE (IFCBOOLEAN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "Ziegel 200" (IFCIDENTIFIER)
    ThermalTransmittance = 2.7 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Ziegel+WD hart 300+160" (IFCIDENTIFIER)
    ThermalTransmittance = 0.154285714285714 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_WallCommon | properties | on 1 type object
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Ziegel 200" (IFCIDENTIFIER)
    ThermalTransmittance = 2.7 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Pset_OpeningElementCommon | properties | on 8 objects (8 IFCOPENINGELEMENT)
    Reference = "Ziegel+WD hart 300+160" (IFCIDENTIFIER)
  Pset_OpeningElementCommon | properties | on 4 objects (4 IFCOPENINGELEMENT)
    Reference = "Ziegel 200" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "ASN-1" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "EIS-11" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "ESN-1" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "ISN-1" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "RSN-1" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "RSN-1 CE" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "SN-1" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Reference = "TSN-1" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon: 4 more contents on 4 objects not shown
  Pset_ManufacturerTypeInformation | properties | on 12 objects (12 IFCBUILDINGELEMENTPROXY) | on 12 type objects
    Manufacturer = "System Schröders" (IFCLABEL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 0 (IFCINTEGER)

Other addresses and roles
  2 x postal address: "Projektadresse", "Platzl 9", "80331", "München", "Deutschland"